For 1990-2009 cars

### Removal Procedure

1. Remove the following components from the vehicle:

• | The 2 screws (1)

• | The sunshade (2)

2. Remove the following components from the vehicle, if necessary:

• | The screw

• | The sunshade retainer (3)

### Installation Procedure

1. Install the sunshade retainer (3), if removed. Secure the retainer with the screw.
2. Install the sunshade (2) to the vehicle. Secure the sunshade with the 2 screws (1).