For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you review the Steering Wheel and Column-Tilt Description and Operation and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Steering Wheel and Column - Tilt
2 | Attempt to remove the key from the ignition lock cylinder in the OFF position. Did you remove the key from the ignition lock cylinder? | System OK | Go to Step 3
3 | Inspect the lock cylinder for damage. Is the lock cylinder damaged? | Go to Step 5 | Go to Step 4
4 | Inspect the lock cylinder case for damage. Is the lock cylinder or release button damaged? | Go to Step 6 | Go to Step 2
5 | Replace the lock cylinder. Refer to Ignition Lock Cylinder Replacement - On Vehicle . Did you complete the repair? | Go to Step 7 | --
6 | Replace the lock cylinder case. Refer to Ignition Lock Cylinder Case Replacement - On Vehicle . Did you complete the repair? | Go to Step 7 | --
7 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 2