For 1990-2009 cars

## Front Seat Adjuster Track Finish Cover Replacement Outboard

### Removal Procedure

1. Remove the recliner handle (10) from the front seat outboard adjuster (7) by disengaging the retaining tab.
2. Gently pry the outboard adjuster finish cover (9) from the front seat assembly.

### Installation Procedure

1. Install the outboard adjuster finish cover (9) to the front seat assembly.
2. Install the recliner handle (10) to the front seat outboard adjuster (7).

## Front Seat Adjuster Track Finish Cover Replacement Inboard

### Removal Procedure

1. Remove the front floor rear console. Refer to Rear Floor Console Replacement in Instrument Panel, Gages and Console.
2. Remove the following components from the front seat inboard adjuster (3):

• | The screw

• | The inboard adjuster finish cover (2)

### Installation Procedure

1. Install the inboard adjuster finish cover (2) to the front seat inboard adjuster (3). Secure the cover with the screw.
2. Install the front floor rear console. Refer to Rear Floor Console Replacement in Instrument Panel, Gages and Console.