For 1990-2009 cars

Application | Fluid/Lubricant
--- | ---
Automatic Transaxle | DEXRON®-III Automatic Transmission Fluid GM P/N 12346143 (Canadian P/N 10952622) or the equivalent
Chassis Lubrication | Chassis Lubricant GM P/N 12377985, a lubricant meeting the requirements of NLGI # 2, Category LB or GC-LB or the equivalent
Clutch Linkage Pivot Points | Chassis Lubricant GM P/N 12377985, a lubricant meeting the requirements of NLGI # 2, Category LB or GC-LB or the equivalent
Engine Coolant | A 50/50 mixture of clean water (preferably distilled) and a good quality Ethylene Glycol Base CoolantGM P/N 1052753 (Canadian P/N 993089) or equivalent which conforms to GM Specification 1825M, or an approved recycled coolant which conforms to GM Specification 1825M. Refer to Explanation of Scheduled Services .
Engine Oil | The engine oil with the American Petroleum Institute Certified For Gasoline Engines "Starburst" symbol of the correct viscosity. In order to determine the preferred viscosity for your vehicle's engine, refer to Explanation of Scheduled Services .
Floor Shift Linkage | Lubriplate® Lubricant Aerosol GM P/N 12346293, a lubricant meeting the requirements of NLGI # 2, Category LB or GC-LB or the equivalent
Hood and Door Hinges | Multi-Purpose Lubricant, Superlube®, GM P/N 12346241 (Canadian P/N 10953474) or the equivalent.
Hood Latch Assembly, Secondary Latch Assembly, Pivots, Spring Anchor and Release Pawl | Lubriplate® Lubricant Aerosol GM P/N 12346293, a lubricant meeting the requirements of NLGI # 2, Category LB or GC-LB or the equivalent
Hydraulic Brake System | Delco Supreme 11® Brake Fluid GM P/N 12377967 (Canadian 992667) or an equivalent DOT-3 brake fluid
Hydraulic Clutch System | Hydraulic Clutch Fluid GM P/N 12345347 (Canadian P/N 10953517) or the equivalent
Key Lock Cylinders | Multi-Purpose Lubricant, Superlube®, GM P/N 12346241 (Canadian P/N 10953474) or the equivalent.
Manual Transaxle | GM Goodwrench Synthetic Manual Transmission Fluid GM P/N 12346190 (Canadian P/N 10953477) or an equivalent SAE 75W-90 GL-4 Gear Oil.
Manual Transaxle Shift Linkage | Chassis Lubricant GM P/N 12377985, a lubricant meeting the requirements of NLGI # 2, Category LB or GC-LB or the equivalent
Weatherstrip Conditioning | Dielectric Silicone Grease GM P/N 12345579 (Canadian P/N 1974984), or Weatherstrip Lubricant-Krytox (GM P/N 3634770) or the equivalent.
Windshield Washer Solvent | GM Optikleen® Washer Solvent GM P/N 1051515 (Canadian P/N 993033) or the equivalent.