For 1990-2009 cars

### Removal Procedure

1. Remove the IP accessory center trim plate. Refer to Instrument Panel Center Trim Panel Replacement in Instrument Panel, Gauges and Console.
2. Remove the 4 screws (2) which secure the radio (1).
3. Pull the radio (2) from the instrument panel.
4. Disconnect the following from the radio:

• | The electrical connector

• | The antenna lead (1)

### Installation Procedure

1. Connect the radio electrical connector.
2. Connect the antenna lead (1) to the radio (2).
3. Install the radio (1) to the instrument panel. Secure the radio with the 4 screws (2).
4. Install the IP accessory center trim plate. Refer to Instrument Panel Center Trim Panel Replacement in Instrument Panel, Gauges and Console.