For 1990-2009 cars

Checks | Causes
--- | ---
Engine Mounts | Loose or worn
Pressure Plate |

• | Warped pressure plate surface

• | Burned or smeared resin on pressure plate surface

Clutch Disc |

• | Oil contamination

• | Excessively worn, exploded or damaged disc

• | Worn or broken torsion springs

• | Worn splines in the disc hub

Flywheel |

• | Flywheel surface runout

• | Burned or smeared resin on the flywheel surface

Transaxle Input Shaft | Worn or damaged splines