For 1990-2009 cars

#### Fluid Capacities (Approximate)

Application | Specification
--- | ---
Metric | English
Pan Removal | 3.1 liters | 3.3 quarts
Overhaul Less Torque Converter | 7.6 liters | 8.0 quarts
The fluid recommended for this vehicle is Dexron® -III Automatic Transmission Fluid

Application | Specification
--- | ---
Metric | English
Fluid Recommended | Dexron®-III Automatic Transmission Fluid GM P/N 12346143 or equivalent
Overhaul Less Torque Converter | 3.5 liters | 3.7 qts
Overhaul with New Torque Converter | 4.9 liters | 5.2 qts
Pan Removal | 1.5 liters | 1.6 qts