For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you review the Power Steering System Description and Operation and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Power Steering System
2 | Verify that power steering fluid leaks are present. Is the power steering system leaking? | Go to Step 3 | System OK
3 | Inspect the power steering system fittings. Are the fittings leaking? | Go to Step 8 | Go to Step 4
4 | Inspect the power steering hoses. Are the hoses leaking? | Go to Step 9 | Go to Step 5
5 | Inspect the power steering fluid reservoir for leaks. Is the reservoir leaking? | Go to Step 10 | Go to Step 6
6 | Inspect the power steering pump for leaks. Is the power steering pump leaking? | Go to Step 11 | Go to Step 7
7 | Inspect the power steering gear for leaks. Is the power steering gear leaking? | Go to Step 12 | Go to Step 8
8 | Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

Replace the hose clamps, if necessary. Tighten the fittings. Refer to Fastener Tightening Specifications .

Did you complete the repair?

Go to Step 13

--

9 | Replace the power steering hoses. Refer to the following procedures:

• | Power Steering Fluid Reservoir Inlet Hose Replacement

• | Power Steering Fluid Reservoir Outlet Hose Replacement

• | Power Steering Gear Inlet Pipe Replacement

• | Power Steering Gear Outlet Pipe Replacement

Did you complete the repair?

Go to Step 13

--

10 | Replace the power steering fluid reservoir. Refer to Remote Power Steering Fluid Reservoir Replacement . Did you complete the repair? | Go to Step 13 | --
11 | Replace the power steering pump. Refer to Power Steering Pump Replacement . Did you complete the repair? | Go to Step 13 | --
12 | Replace the power steering gear. Refer to Steering Gear Replacement . Did you complete the repair? | Go to Step 13 | --
13 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 3