For 1990-2009 cars

Figure 1: |

#### Junction Block 1

(1) | Junction Block 1 C5
(2) | Junction Block 1 C7 (on backside)
(3) | Junction Block 1 C3
(4) | Junction Block 1 C2
(5) | Junction Block 1 C1
(6) | Flasher Relay
(7) | C/OPN Relay
(8) | P/W Relay
(9) | Junction Block 1
(10) | Junction Block 1 C6 (on backside)
(11) | Junction Block 1 C4

Figure 2: |

#### Junction Block 2

(1) | Not Used
(2) | ST Fuse 5A
(3) | D/L Fuse 30A
(4) | Fog Fuse 15A
(5) | S-HTR Fuse 15A
(6) | Not Used
(7) | CIG Fuse 15A
(8) | DEF Fuse 40A
(9) | Dome Noise Filter
(10) | POWER Fuse 30A
(11) | Short Pin
(12) | C2
(13) | C5
(14) | C4
(15) | ECU-B Fuse 7.5A
(16) | C3
(17) | C1
(18) | Not Used
(19) | DEF-I/UP Fuse 10A
(20) | WIP Fuse 20A
(21) | GAUGE Fuse 10A
(22) | Not Used
(23) | TURN Fuse 7.5A
(24) | STOP Fuse 15A
(25) | IGN Fuse 7.5A
(26) | TAIL Fuse 15A
(27) | ECU-IG Fuse 10A
(28) | OBD Fuse 7.5A
(29) | Not Used

Figure 3: |

#### Fuse and Relay Block 1

(1) | ST Relay
(2) | HEAD Relay
(3) | EFI or F-HTR Relay
(4) | Fuse Puller
(5) | ENGINE MAIN Relay
(6) | HORN Relay
(7) | AM1 Fuse 50A
(8) | RDI Fuse 30A
(9) | FAN Relay
(10) | ALT-S Fuse 7.5A
(11) | Empty
(12) | Not Used
(13) | HORN Fuse 20A
(14) | Not Used
(15) | Not Used
(16) | AM2 Fuse 30A
(17) | HAZARD Fuse 20A
(18) | DOME Fuse 20A
(19) | ALT Fuse 100A
(20) | ABS Fuse 50A
(21) | MAIN Fuse 50A
(22) | Not Used
(23) | Fuse and Relay Block 1

Figure 4: |

#### Fuse and Relay Block 2

(1) | A/C MG Relay
(2) | A/C FAN No.3 Relay
(3) | A/C FAN No.3 Relay
(4) | Dimmer Relay
(5) | CDS Fuse 30A
(6) | HEAD (LH-LWR) Fuse 10A
(7) | HEAD (RH-LWR) Fuse 10A
(8) | DRL Fuse 7.5A
(9) | Fuse and Relay Block 2

Figure 5: |

#### Fuse and Relay Block 3

(1) | HTR Fuse 50A
(2) | HTR Relay
(3) | DRL Relay
(4) | Fuse and Relay Block 3
(5) | A/C Fuse 7.5A

Figure 6: |

#### Engine Compartment View

(1) | Spark Plug 4
(2) | Ignition Coil 1
(3) | Ignition Coil 2
(4) | Brake Pressure Modulator Valve (BPMV)
(5) | Data Link Connector (Underhood)
(6) | Ambient Light Sensor
(7) | Intake Temperature (IAT) Sensor
(8) | Fuse and Relay Block 1
(9) | Fuse and Relay Block 2
(10) | Battery
(11) | Throttle Position (TP) Sensor (In Back)
(12) | Throttle Linkage
(13) | Horn
(14) | Camshaft Position (CMP) Sensor Right Rear of Cylinder Head
(15) | Ambient Air Temperature Sensor (Tachometer Only)
(16) | Auxiliary Radiator Fan Motor (Attached to Rear of Radiator) (With A/C Only)
(17) | Knock Sensor
(18) | A/C Compressor Clutch (Below Generator)
(19) | Refrigerant Pressure Switch (With A/C Only)
(20) | Fuse and Relay Block 3
(21) | Generator
(22) | A/C Accumulator (With A/C Only)
(23) | Windshield Washer Pump
(24) | Windshield Wiper Motor
(25) | Cruise Control Servo
(26) | Spark Plug 1
(27) | Spark Plug 2
(28) | Spark Plug 3

Figure 7: |

#### Instrument Panel Assembly (Left Side)

(1) | Hazard Switch
(2) | Rear Defogger Switch
(3) | Overdrive Switch
(4) | Radio
(5) | Junction Block 2
(6) | OBD II DLC
(7) | Junction Block 1
(8) | Multifunction Alarm Module
(9) | Outside Rearview Mirror Controller
(10) | IP Lamp Dimmer
(11) | Ignition Switch
(12) | Junction Block 3

Figure 8: |

#### Passthrough and Ground Views

(1) | G200
(2) | P500
(3) | P100
(4) | P102
(5) | G101
(6) | G100
(7) | G103
(8) | G105, G106
(9) | G104
(10) | P101
(11) | P600
(12) | G203
(13) | P800
(14) | G301
(15) | P301
(16) | G400
(17) | G300
(18) | P300
(19) | G202
(20) | P700
(21) | G201, G204