For 1990-2009 cars

### Operation

The optional sunroof features both tilt and sliding capabilities. When the TILT UP switch (1) is pressed, the rear edge of the sunroof will raise up. The sunroof must be completely closed before tilt operation can be accomplished. When the sunroof is in the tilted position, it must be closed before sliding operation can be accomplished. When the SLIDE switch (2) is pressed, the sunroof will slide rearward. When the sunroof is open and the SLIDE switch (2) is pressed, the sunroof will slide forward but will stop short of being completely closed. The SLIDE switch (2) must be pressed a second time to completely close the sunroof.