For 1990-2009 cars

### Removal Procedure

1. Open the rear side door.
2. Beginning at the bottom of the roof rear drip molding (1), gently pull up to release the 3 plastic retainers which secure the molding.
3. Remove the roof rear drip molding (1) from the vehicle.

### Installation Procedure

1. Install the roof rear drip molding (1) to the vehicle. Ensure that the plastic retainers are completely engaged.
2. Close the rear side door.