For 1990-2009 cars

### Removal Procedure

1. Remove the IP accessory center trim plate. Refer to Instrument Panel Center Trim Panel Replacement in Instrument Panel, Gages, and Console.
2. Remove the IP ashtray illumination lamp socket (2) from the ashtray housing (3).
3. Remove the ashtray illumination bulb (1) from the lamp socket (2).

### Installation Procedure

1. Install the IP ashtray illumination bulb (1) to the lamp socket (2).
2. Install the ashtray illumination lamp socket (2) to the ashtray housing (3).
3. Install the IP accessory center trim plate. Refer to Instrument Panel Center Trim Panel Replacement in Instrument Panel, Gages, and Console.