For 1990-2009 cars

## Data Link Communications Connector End Views Data Link Connnector (Under Hood)

#### Data Link Connector (Under Hood)

Connector Part Information |

• | 90980-11195

• | BLK

Pin | Wire Color | Function
--- | --- | ---
FP | -- | Not Used
W | -- | Not Used
E1 | BRN | Ground
OX1 | -- | Not Used
AB | BLK/YEL | AIR BAG Indicator Control
OP1 | -- | Not Used
CCO | -- | Not Used
TE1 | BLU/WHT | Diagnostic Request (PCM)
TE2 | -- | Not Used
CC2 | -- | Not Used
TC | PNK/BLK | Diagnostic Request (SDM/BPMV)
TB | BLK | EFI Relay Output
VF1 | -- | Not Used
VF2 | -- | Not Used
OX2 | -- | Not Used
TS | BLU | Diagnostic Request (BPMV)
TT | -- | Not Used
OP4 | -- | Not Used
IG | -- | Not Used
OP2 | -- | Not Used
OP3 | -- | Not Used
WA | -- | Not Used
WB | -- | Not Used

## Data Link Communications Connector End Views Data Link Connector OBD 2

#### (DLC) OBD 2

Connector Part Information |

• | 90980-11665

• | WHT

Pin | Wire Color | Function
--- | --- | ---
1-3 | -- | Not Used
4 | WHT/BLK | Ground
5 | BRN | Ground
6 | -- | Not Used
7 | WHT | Serial Data
8-15 | -- | Not Used
16 | RED | Battery Positive Voltage