For 1990-2009 cars

### Removal Procedure

1. Disable the SIR system. Refer to Disabling the SIR System .
2. Remove the driver front seat back cover. Refer to Front Seat Back Cushion Cover and Cushion Pad Replacement in Seats.
3. Disconnect the inflatable restraint side impact module electrical connector (3).
4. Remove the inflatable restraint side impact module fasteners (1).
5. Remove the inflatable restraint side impact module (2).

### Installation Procedure

1. Install the inflatable restraint side impact module (2).
2. Install the inflatable restraint side impact module fasteners (1).
3. Connect the inflatable restraint side impact module electrical connector (3).
4. Install the driver front seat back cover. Refer to Front Seat Back Cushion Cover and Cushion Pad Replacement in Seats.
5. Enable the SIR system. Refer to Enabling the SIR System .