For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Booster Assembly Mounting Nut | 13 N·m | 108 lb in
Brake Hose Bolt | 8 N·m | 71 lb in
Brake Pedal Bracket Front Bolt | 20 N·m | 14.75 lb ft
Brake Pedal Bracket Nut | 10 N·m | 89 lb in
Brake Pedal Shaft Bolt and Nut | 20 N·m | 14.75 lb ft
Clevis Lock Nut | 26 N·m | 19 lb ft
Front Brake Hose Retaining Bracket Bolt | 15 N·m | 11 lb ft
Knee Bolster Bolt | 10 N·m | 89 lb in
Knee Bolster Trim Panel Bolt | 10 N·m | 89 lb in
LH Kick Panel Nut | 5.4 N·m | 48 lb in
Master Cylinder Mounting Nuts | 13 N·m | 108 lb in
Master Cylinder Nuts | 13 N·m | 108 lb in
Piston Stopper Bolt | 10 N·m | 89 lb in
Proportioning Valve Bolt | 10 N·m | 89 lb in
Stoplamp Switch Locknut | 10 N·m | 89 lb in