For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
DEFINITION: The steering wheel and column tilts, but the tilt lever does not hold the column in one position.
1 | Did you review the Steering Wheel and Column-Tilt Description and Operation and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Steering Wheel and Column - Tilt
2 | Verify that the steering wheel and column does not lock in any tilt postion. Does the steering wheel and column lock in any tilt position? | System OK | Go to Step 3
3 | Replace the steering column. Refer to Steering Column Replacement . Did you complete the repair? | Go to Step 4 | --
4 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 3