For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Crossmember Front Outer Bolts | 225 N·m | 167 lb ft
Engine Crossmember-to-Suspension Crossmember Nut and Bolt | 60 N·m | 45 lb ft
Engine Splash Shield Bolts | 10 N·m | 89 lb in
Front Suspension Crossmember Nuts | 57 N·m | 42 lb ft
Front Transaxle Mount Bolts | 64 N·m | 47 lb ft
Left or Right Control Arm Retaining Bracket Inner Bolt | 175 N·m | 129 lb ft
Left or Right Control Arm Retaining Bracket Outer Bolt | 147 N·m | 109 lb ft
Left or Right Control Arm Retaining Bracket Rear Bolt | 123 N·m | 91 lb ft
Stabilizer Shaft Mounting Bracket Stud | 147 N·m | 109 lb ft
Suspension Support Brace Nut | 69 N·m | 51 lb ft