For 1990-2009 cars

### Removal Procedure

1. Pull the sunshade (2) from the sunshade support (1) and position the sunshade to the side of the vehicle.
2. Remove the 2 screws which secure the sunshade (2).
3. Remove the sunshade from the vehicle.
4. Remove the screw which secures the sunshade support (1), if necessary.
5. Remove the support from the vehicle, if necessary.

### Installation Procedure

1. Install the sunshade support (1) to the vehicle, if removed. Secure the support with 1 screw.
2. Install the sunshade (2) to the vehicle. Secure the sunshade with the 2 screws.
3. Install the sunshade (2) to the sunshade anchor (1).