For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
4-Speed Automatic Transmission (RPO M41)

- Bottom Pan Removal

2.5 liters

2.6 quarts

- Complete Overhaul (1.6 L)

6.9 liters

7.3 quarts

- Complete Overhaul (2.0 L)

7.1 liters

7.5 quarts

5-Speed Manual Transmission (RPO M59)

- Two-Wheel-Drive Models

1.9 liters

2.0 quarts

- Four-Wheel-Drive Models

1.5 liters

1.6 quarts

- Transfer Case (Four-Wheel-Drive Only)

1.7 liters

1.8 quarts

Axle Housing

- Front

1.0 liters

1.1 quarts

- Rear

2.2 liters

2.3 quarts

Cooling System Capacity

- 1.6L Engine

5.5 liters

5.8 quarts

- 2.0L Engine

6.5 liters

6.9 quarts

Engine Crankcase

- Without Filter Change 1.6L Engine

4.0 liters

4.2 quarts

- Without Filter Change 2.0L Engine

5.0 liters

5.3 quarts

- With Filter Change 1.6L Engine

4.2 liters

4.4 quarts

- With Filter Change 2.0L Engine

5.2 liters

5.5 quarts

Fuel Tank

- 2-Door Models

56.0 liters

14.8 gallons

- 4-Door Models

66.0 liters

17.4 gallons