For 1990-2009 cars

The rear window is made of a very pliable plastic material which is easily scratched. Observer the following precautions in order to prevent damage to the rear window:

• | Use the following guidelines when wiping dust from the rear window:

- | use a soft cotton cloth moistened with clean lukewarm or cold water.

- | Move the cloth in one direction without stopping.

- | Never use a dry cloth.

• | Use the following guidelines when removing frost, snow, or ice from the rear window:

- | Use lukewarm water.

- | Do not use a scraper or de-icing chemicals in order to remove ice from the rear window.

• | Use the following guidelines in order to wash the rear window:

- | Use lukewarm or cold water.

- | Do not use hot water or any detergents in order to wash the rear window.

- | Do not use solvents such as alcohol or harsh cleaning agents.

- | Rinse the rear window.

- | Wipe the window with a moistened clean soft cloth.

• | Use the following guidelines for stickers, tape, or gummed labels applied to the rear window:

- | Do not paste stickers, gummed labels, or apply tape to the rear windows.

- | Removing adhesives remains from labels, stickers, or tape from the rear window is very difficult.

- | Using solvents or forcibly removing adhesive may damage the rear window.

- | Use a repeated sticking-and-removing action with another new sticker or tape if the adhesive remains are soft.