For 1990-2009 cars

### Removal Procedure

1. Swing the sunshade down in order to gain access to the folding top latch (1).
2. Push in the folding top latch buttons (2).
3. Pull the latch (1) back in order to unhook the latch (1) from the folding top #1 bow.
4. Remove the 2 screws which secure the folding top latch.
5. Remove the folding top latch from the vehicle.

### Installation Procedure

1. Install the folding top latch to the vehicle. Secure the latch with the 2 screws.
2. Hook the folding top #1 bow to the folding top latches (1).
3. Push the latch (1) down until the latch clicks into place.
4. Return the sunshade back to their original position.