For 1990-2009 cars

## Front Floor Panel Carpet Replacement 4 Door

### Removal Procedure

1. Remove the front seats Refer to Front Seat Replacement - Bucket in Seats.
2. Remove the rear floor console. Refer to Rear Floor Console Replacement in Instrument Panel, Gauges and Console.
3. Remove the front floor console. Refer to Front Floor Console Replacement in Instrument Panel, Gauges and Console.
4. Remove the front floor foot rest. Refer to Foot Rest Replacement .
5. Remove the following components from the vehicle:

5.1. | The 3 plastic retainers (2)

5.2. | The front side door sill trim plate (1)

6. Remove the body hinge pillar trim panels. Refer to Body Hinge Pillar Trim Panel Replacement .
7. Remove the following components from the vehicle:

7.1. | The 3 plastic retainers

7.2. | The rear side door sill trim plate

8. Remove the lower center pillar trim panel. Refer to Center Pillar Lower Trim Panel Replacement .
9. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement in Seats.
10. Remove the 2 plastic retainers (2) which secure each side of the front floor panel carpet (1) to the bulkhead.
11. Remove the front floor panel carpet (1) from the vehicle.

### Installation Procedure

1. Install the front floor panel carpet (1) to the vehicle.
2. Install the 2 plastic retainers (2) which secure each side of the front floor panel carpet (1) to the bulkhead.
3. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement in Seats.
4. Install the lower center pillar trim panel. Refer to Center Pillar Lower Trim Panel Replacement .
5. Install the rear side door sill trim plate to the vehicle. Secure the trim plate with the 3 plastic retainers.
6. Install the body hinge pillar trim panels. Refer to Body Hinge Pillar Trim Panel Replacement .
7. Install the front side door sill trim plate (1) to the vehicle. Secure the trim plate with the 3 plastic retainers (2).
8. Install the front floor foot rest. Refer to Foot Rest Replacement .
9. Install the front floor console. Refer to Front Floor Console Replacement in Instrument Panel, Gauges and Console.
10. Install the rear floor console. Refer to Rear Floor Console Replacement in Instrument Panel, Gauges and Console.
11. Install the front seats Refer to Front Seat Replacement - Bucket in Seats.

## Front Floor Panel Carpet Replacement 2 Door

### Removal Procedure

1. Remove the front seats Refer to Front Seat Replacement - Bucket in Seats.
2. Remove the rear floor console. Refer to Rear Floor Console Replacement in Instrument Panel, Gauges and Console.
3. Remove the front floor console. Refer to Front Floor Console Replacement in Instrument Panel, Gauges and Console.
4. Remove the front floor foot rest. Refer to Foot Rest Replacement .
5. Remove the following components from each side of the vehicle:

5.1. | The 4 plastic retainers (2)

5.2. | The front side door sill trim plate (1)

6. Remove the body hinge pillar trim panels. Refer to Body Hinge Pillar Trim Panel Replacement .
7. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement in Seats.
8. Remove the 2 plastic retainers (2) which secure each side of the front floor panel carpet (1) to the bulkhead.
9. Remove the front floor panel carpet (1) from the vehicle.

### Installation Procedure

1. Install the front floor panel carpet (1) to the vehicle.
2. Install the 2 plastic retainers (2) which secure each side of the front floor panel carpet (1) to the bulkhead.
3. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement in Seats.
4. Install the body hinge pillar trim panels. Refer to Body Hinge Pillar Trim Panel Replacement .
5. Install the front side door sill trim plate (1) to the vehicle. Secure the trim plate with the 4 plastic retainers (2).
6. Install the front floor foot rest. Refer to Foot Rest Replacement .
7. Install the front floor console. Refer to Front Floor Console Replacement in Instrument Panel, Gauges and Console.
8. Install the rear floor console. Refer to Rear Floor Console Replacement in Instrument Panel, Gauges and Console.
9. Install the front seats Refer to Front Seat Replacement - Bucket in Seats.