For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
DEFINITION: The clutch engages but slips while driving the vehicle.
1 | Check the clutch release system in order to ensure that it is working properly. Is the clutch release system working properly? | Go to Step 2 | Go to Step 7
2 | Check the clutch disc for overheating. Is the clutch disc overheated? | Go to Step 3 | Go to Step 5
3 | Allow the disc plate to cool. Does the clutch still slip? | Go to Step 4 | System OK
4 | Check the clutch disc in order to see if the disc is oil soaked. Is the disc plate oil soaked? | Go to Step 5 | Go to Step 7
5 | Correct the leak at the source and replace the clutch disc. Refer to Clutch Assembly Replacement . Does the clutch still slip? | Go to Step 6 | System OK
6 | Check for a warped clutch cover on the disc plate or a weak diaphragm spring. Is the disc plate warped or the diaphragm spring weak? | Go to Step 7 | --
7 | Replace the necessary components. Does the clutch still slip? | -- | System OK