For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Blower Motor | Behind the RH instrument panel | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges and Console | --
Blower Motor Resistor | Behind the RH instrument panel at the top of the blower motor housing | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges and Console | --
Blower Speed Selector Switch | Center of the instrument panel above the radio | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges and Console | --
Fuse Block 2 | Under the LH instrument panel | Power and Grounding Component Views in Wiring Systems | --
C217 (6 Cavities) | Main harness to the blower speed selector switch, RH instrument panel | Harness Routing Views in Wiring Systems | --
G201 | Behind the RH instrument panel near the blower assembly | Power and Grounding Component Views in Wiring Systems | --
S209 | Main harness, approximately 12 cm from the blower speed selector switch connector breakout | Harness Routing Views in Wiring Systems | --
S228 | Main harness, approximately 4 cm from the C212 breakout | Harness Routing Views in Wiring Systems | --
S239 | Main harness, approximately 2 cm from the daytime running lamps (DRL) diode breakout | Harness Routing Views in Wiring Systems | --