For 1990-2009 cars

Figure 1: |

#### Engine 1.6L Components

(1) | Fuel Sender Assembly
(2) | Camshaft Position (CMP) Sensor
(3) | Heated Oxygen Sensor 2 (HO2S2)
(4) | Ignition Coils
(5) | Front Wiper Motor
(6) | Electronic Brake Control Module (EBCM)
(7) | Cruise Control Servo
(8) | Heated Oxygen Sensor 1 (HO2S1)
(9) | Power Steering Pressure Switch
(10) | Fuel Injectors
(11) | Crankshaft Position (CKP) Sensor
(12) | Engine Coolant Temperature (ECT) Sensor
(13) | Intake Air Control (IAC) Valve
(14) | Throttle Position (TP) Sensor
(15) | EVAP Canister Purge Valve
(16) | EVAP Canister
(17) | EVAP Canister Vent Solenoid
(18) | Mass Air Flow (MAF) Sensor
(19) | Intake Air Temperature (IAT) Sensor
(20) | A/C Condenser Fan Relay
(21) | Battery
(22) | Exhaust Gas Recirculation (EGR) Valve
(23) | Manifold Absolute Pressure (MAP) Sensor
(24) | Transmission Range Switch
(25) | Vehicle Speed Sensor
(26) | Fuel Tank Pressure Sensor

Figure 2: |

#### Engine 2.0L Components

(1) | Engine Coolant Temperature (ECT) Sensor
(2) | Camshaft Position (CMP) Sensor
(3) | Ignition Coils
(4) | Front Wiper Motor
(5) | Electronic Brake Control Module (EBCM)
(6) | Front Washer Pump
(7) | Rear Washer Pump
(8) | Brake Fluid Level Switch
(9) | Heated Oxygen Sensor 1 (HO2S1)
(10) | Heated Oxygen Sensor 2 (HO2S2)
(11) | Power Steering Pressure Switch
(12) | EVAP Canister Purge Valve
(13) | EVAP Canister
(14) | EVAP Canister Vent Solenoid
(15) | Mass Air Flow (MAF) Sensor
(16) | Intake Air Temperature (IAT) Sensor
(17) | Fuse Block
(18) | A/C Condenser Fan Relay
(19) | EVAP Tank Pressure Control Solenoid Valve
(20) | Battery
(21) | Crankshaft Position (CKP) Sensor
(22) | Intake Air Control (IAC) Valve
(23) | Throttle Position (TP) Sensor
(24) | Exhaust Gas Recirculation (EGR) Valve
(25) | Manifold Absolute Pressure (MAP) Sensor
(26) | Fuel Injectors

Figure 3: |

#### Instrument Cluster (Rear View)

(1) | Instrument Cluster

Figure 4: |

#### Fuel Tank

(1) | Fuel Tank Pressure Sensor
(2) | Fuel Sender Assembly
(3) | Fuel Tank