For 1990-2009 cars

### Removal Procedure

1. Remove the instrument cluster. Refer to Instrument Cluster Replacement .
2. Release the 6 plastic clear tabs which secure the instrument cluster lens (2) to the instrument cluster bezel (1).

### Installation Procedure

1. Install the instrument cluster lens (2) to the instrument cluster bezel (1) by pressing around the lens until the tabs snap into place.
2. Install the instrument cluster. Refer to Instrument Cluster Replacement .