For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Disc Brake Pad Lining and Plate Thickness, New | 15.5 mm | 0.610 in
Disc Brake Pad Lining and Plate Thickness, Minimum | 7.5 mm | 0.295 in
Disc Brake Pad Lining Thickness, New | 10.0 mm | 0.390 in
Disc Brake Pad Lining Thickness, Minimum | 2.0 mm | 0.080 in
Rotor Lateral Runout, Maximum | 0.15 mm | 0.006 in
Rotor Surface Finish Scoring Depth, Maximum | 0.38 mm | 0.015 in
Rotor Thickness, New | 17 mm | 0.670 in
Rotor Thickness, Minimum | 15 mm | 0.590 in
Rotor Thickness Variation, Maximum | 0.013 mm | 0.0005 in