For 1990-2009 cars

#### Tools Required

• | J 8763-B Holding Fixture

• | J 3289-20 Holding Fixture Base

Notice: Excessive tightening of the holding fixture onto the transmission assembly could cause damage and inhibit disassembly.

1. Install J 8763-B onto the transmission assembly.
2. Install the transmission assembly and J 8763-B into J 3289-20 and use the fixture pin to lock the holding fixture in place.