For 1990-2009 cars

Application | Liters (L) | Gallons (gal) | Quarts (qt)
--- | --- | --- | ---
3-Speed Automatic Transmission (RPO M65)

- Pan Removal

2.8

--

3.0

- Overhaul including Torque Convertor Clutch

5.1

--

5.3

4-Speed Automatic Transmission (RPO M65)

- Pan Removal

2.5

--

2.64

- Overhaul including Torque Converter Clutch

6.9

--

7.3

Axle Housing

- Front

1.0

--

1.1

- Rear

2.2

--

2.3

Cooling System Capacity

- Models with Automatic Transmission

5.2

--

5.5

- Models with Manual Transmission

5.3

--

5.6

Engine Crankcase

- With Filter Change

4.2

--

4.5

- Without Filter Change

4.0

--

4.2

Fuel Tank

- 2-Door Models

42.0

11.0

--

- 4-Door Models

55.0

14.5

--

Manual Transmission

- Two-Wheel-Drive Models

1.9

--

2.0

- Four-Wheel-Drive Models

1.5

--

1.6

- Transfer Case

1.7

--

1.8