For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Distributor | Top rear of the engine | Engine Controls Component Views in engine controls | --
Engine Coolant Temperature (ECT) Sending Unit | RH side of the engine in the thermostat housing | Instrument Panel, Gages, and Console Component Views | --
Fuel Level Sensor | In the fuel tank | Engine Controls Component Views in engine controls | --
Fuse Block 2 | Under the LH instrument panel | Power and Grounding Component Views in Wiring Systems | --
Instrument Panel Cluster Assembly | LH instrument panel | -- | --
C1 (16 Terminals) | Instrument panel harness to the instrument panel cluster assembly behind the instrument panel cluster assembly | Instrument Panel, Gages, and Console Component Views | --
C2 (10 Terminals) | Instrument panel harness to the instrument panel cluster assembly behind the instrument panel cluster assembly | Instrument Panel, Gages, and Console Component Views | --
C3 (13 Terminals) | Instrument panel harness to the instrument panel cluster assembly behind the instrument panel cluster assembly | Instrument Panel, Gages, and Console Component Views | --
Noise Suppressor Filter | LH rear engine compartment below the front wiper motor | Engine Controls Component Views in engine controls | --
Oil Pressure Switch | LH engine above the oil filter | Instrument Panel, Gages, and Console Component Views | --
Powertrain Control Module (PCM) | Under the LH instrument panel to the left of the steering column | Engine Controls Component Views in engine controls | Powertrain Control Module Connector End Views in Engine controls
3-Speed Automatic and Manual Transmissions C1 (22 Cavities) | Main harness to the PCM, behind the instrument panel to the left of the steering column | -- | --
3-Speed Automatic and Manual Transmissions C2 (16 Cavities) | Main harness to the PCM, behind the instrument panel to the left of the steering column | -- | --
3-Speed Automatic and Manual Transmissions C3 (26 Cavities) | Main harness to the PCM, behind the instrument panel to the left of the steering column | -- | --
4-Speed Automatic and Manual Transmissions C1 (22 Cavities) | Main harness to the PCM, behind the instrument panel to the left of the steering column | -- | --
4-Speed Automatic and Manual Transmissions C2 (12 Cavities) | Main harness to the PCM, behind the instrument panel to the left of the steering column | -- | --
4-Speed Automatic and Manual Transmissions C3 (16 Cavities) | Main harness to the PCM, behind the instrument panel to the left of the steering column | -- | --
4-Speed Automatic and Manual Transmissions C4 (26 Cavities) | Main harness to the PCM, behind the instrument panel to the left of the steering column | -- | --
C100 (16 Cavities) | Main harness to the engine harness mounted to the bracket on the bulkhead to the left of the front wiper motor | Harness Routing Views in wiring systems | --
C101 (16 Cavities) | Main harness to the engine harness mounted to the bracket on the bulkhead to the left of the front wiper motor | Harness Routing Views in wiring systems | --
C200 (22 Cavities) | Main harness to the instrument panel harness, LH instrument panel near fuse block 2 | Harness Routing Views in wiring systems | --
C201 (16 Cavities) | Main harness to the instrument panel harness, LH instrument panel near fuse block 2 | Harness Routing Views in wiring systems | --
C202 (22 Cavities) | Main harness to the floor harness, LH instrument panel near G200 | Harness Routing Views in wiring systems | --
C211 (16 Cavities) | Instrument panel harness to the floor harness, RH instrument panel near the A-pillar | Harness Routing Views in wiring systems | --
C400 (12 Cavities) | Floor harness to the rear lamp harness behind the LH rear wheelhousing | Harness Routing Views in wiring systems | --
C404 (1 Cavity) | Rear lamp harness to the rear door harness behind the RH rear wheelhousing | Harness Routing Views in wiring systems | --
G101 | On the bulkhead behind the distributor | Power and Grounding Component Views in Wiring Systems | --
G102 | RH rear of the engine near the distributor | Power and Grounding Component Views in Wiring Systems | --
G200 | Behind the LH instrument panel above fuse block 2 | Power and Grounding Component Views in Wiring Systems | --
G400 (4-Door) | Inside the rear door near the license plate lamps | Power and Grounding Component Views in Wiring Systems | --
G400 (2-Door) | Inside the rear door near the license plate lamps | Power and Grounding Component Views in Wiring Systems | --
P200 | LH rear engine compartment on the bulkhead near the brake master cylinder | Power and Grounding Component Views in Wiring Systems | --
P300 (2-Door) | LH A-pillar under the instrument panel behind the LH kick panel | Power and Grounding Component Views in Wiring Systems | --
P400 (2-Door) | Rear door | Power and Grounding Component Views in Wiring Systems | --
P400 (4-Door) | Rear door | Power and Grounding Component Views in Wiring Systems | --
P401 | Rear of the vehicle to the right of the LH frame rail | Power and Grounding Component Views in Wiring Systems | --
P402 | Rear of the vehicle to the left of the RH frame rail | Power and Grounding Component Views in Wiring Systems | --
S106 | Main harness, approximately 10 cm (3.93 in) from the noise suppressor filter connector breakout | Harness Routing Views in Wiring Systems | --
S130 | Main harness approximately 20 cm (7.87 in) from the noise suppressor filter connector breakout | Harness Routing Views in Wiring Systems | --
S132 | Main harness approximately 7 cm (2.75 in) from the noise suppressor filter connector breakout | Harness Routing Views in Wiring Systems | --
S204 | Instrument panel harness near the C211 breakout | Harness Routing Views in Wiring Systems | --
S226 | Instrument panel harness near the radio breakout | Harness Routing Views in Wiring Systems | --
S230 | Main harness approximately 5 cm (1.96 in) from the G300 breakout | Harness Routing Views in Wiring Systems | --
S262 | Main harness approximately 8 cm (3.14 in) from the stoplamp switch connector breakout | Harness Routing Views in Wiring Systems | --
S272 | Main harness approximately 11 cm (4.33 in) from the G200 breakout | Harness Routing Views in Wiring Systems | --
S305 (2-Door) | Floor harness approximately 20 cm (7.87 in) from the LH rear speaker connector breakout | Harness Routing Views in Wiring Systems | --
S400 | Rear door harness near G400 breakout | Harness Routing Views in Wiring Systems | --
S402 | Rear lamp harness, near RH rear combination lamp | Harness Routing Views in Wiring Systems | --
S403 | Rear lamp harness near the RH rear combination lamp | Harness Routing Views in Wiring Systems | --
S419 (4-Door) | Floor harness approximately 50 cm (19.6 in) from the G300 breakout | Harness Routing Views in Wiring Systems | --