For 1990-2009 cars

### Removal Procedure

1. Remove the IP accessory center trim plate. Refer to Instrument Panel Accessory Trim Plate Replacement in Instrument Panel, Gauges and Console.
2. Remove the 4 screws (1) which secure the radio to the instrument panel.
3. Pull the radio (3) forward in order to gain the necessary clearance to disconnect the radio electrical connector (1) and antenna lead (2).
4. Disconnect the electrical connector (1) and antenna lead (2) from the radio (3).
5. Remove the radio (3) from the vehicle.
6. Remove the 4 screws which secure the radio bracket (4) to the radio (3), if necessary.
7. Remove the radio bracket (4) from the radio (3), if necessary.

### Installation Procedure

1. Install the radio bracket (4) to the radio (3), if removed. Secure the bracket with the 4 screws.
2. Connect the antenna lead (2) and electrical connector (1) to the radio (3).
3. Install the radio to the instrument panel. Secure the radio with the 4 screws (1).
4. Install the IP accessory center trim plate. Refer to Instrument Panel Accessory Trim Plate Replacement in Instrument Panel, Gauges and Console.