For 1990-2009 cars

The condition of an automatic transmission not operating properly may be influenced by one or a combination of the following items:

• | The fluid level is high or low. Refer to Automatic Transmission Fluid and Filter Replacement .

• | The engine performance.

• | The TV Cable adjustment. Refer to Automatic Transmission Throttle Valve Cable Adjustment in this section.

• | The shift select cable adjustment.

• | Internal fluid leaks. For complete 03-72LE, 4-speed automatic transmission unit repair procedures, refer to the Transmission/Transaxle/Transfer Case Unit Repair Manual.

• | The electrical system.

• | The transmission or other mechanical components. For complete 03-72LE, 4-speed automatic transmission unit repair procedures, refer to the Transmission/Transaxle/Transfer Case Unit Repair Manual.