For 1990-2009 cars

The reveal moldings for the windshield (4), quarter windows, and the rear door window are a vinyl trim which fits between the edge of the window and the body. The windshield (4) does not need to be removed in order to replace the reveal molding (1). The reveal molding (1) is hand-pressed into place and retained with urethane adhesive. In order to allow room for both the reveal molding and the urethane adhesive to fit in the cavity between the windshield and the body, it may be necessary to trim the reveal molding (1). The rear door window or quarters windows MUST be removed in order to replace the reveal molding.