For 1990-2009 cars

# Accessory Receptacle is Inoperative (Check Aftermarket Device Plug)

Subject: | Accerssory Receptacle/Cigar Lighter Is Inoperative (Check Aftermarket Device Plug for Short to Ground)

Models: | 1995-2000 Passenger Cars and Trucks

### Condition

Some customers may comment that the cigar lighter or the accessory receptacle is inoperative; or that the internal fuse (within the plug on an aftermarket device), blows intermittently.

### Cause

Certain aftermarket devices have a newly designed power plug with an internal mini fuse. The mini fuse may have an external terminal (which may be used to externally check the fuse). If the mini fuse external test terminal is not recessed into the mini fuse body, it may come in contact with the shell of the vehicle receptacle and cause the fuse (of either the vehicle or the aftermarket device), to blow intermittently.

### Correction

Test the aftermarket device plug for short to ground.

The following step may be performed at the customer's expense. As this is not a defect in material, design or workmanship of the vehicle, it would be the owner's responsibility.

1. Place a piece of tape over the mini fuse terminal temporarily.
2. Explain to the customer that the fuse for the device must have no exposed terminals, and that finding one would be his responsibility.
3. Refer the customer to the manufacturer of the aftermarket device for a new plug.