For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Fuse Block 1 | RH Engine Compartment, front of Battery | Power and Grounding Component Views in Wiring Systems | --
Fuse Block 1 - C1 (3 Cavities) | Main Harness to Fuse Block 1, below Fuse Block 1 | Power and Grounding Component Views in Wiring Systems | --
Fuse Block 2 | Under LH I/P | Power and Grounding Component Views in Wiring Systems | --
Main Relay | Center I/P, behind Blower Speed Selector Switch | Engine Controls Component Views in Engine Controls 1.6L | Powertrain Control Module Connector End Views in Engine Controls 1.6L
Powertrain Control Module (PCM) | Under LH I/P, left of Steering Column | Engine Controls Component Views in Engine Controls 1.6L | --
Powertrain Control Module (PCM) - C1 (22 Cavities) | Main Harness to PCM, behind I/P left of Steering Column | Engine Controls Component Views in Engine Controls 1.6L | --
Torque Converter Clutch (TCC) Relay | RH Engine Compartment, in front of Battery | Engine Controls Component Views in Engine Controls 1.6L | --
Torque Converter Clutch (TCC) Solenoid (Automatic Transmission) | In Transmission, attached to Valve Body | -- | --
C102 (6 Cavities) | Main Harness to Engine Harness, mounted to Bracket on Bulkhead, right of Front Wiper Motor | Harness Routing Views in Wiring Systems | --
C104 (6 Cavities) | Engine Harness to Transmission Harness, under Intake Manifold | Harness Routing Views in Wiring Systems | --
P200 | LH Rear Engine Compartment on Bulkhead, near Brake Master Cylinder | Harness Routing Views in Wiring Systems | --
P201 | RH Rear Engine Compartment on Bulkhead, near Battery | Harness Routing Views in Wiring Systems | --
S142 | Main Harness, approximately 8 cm from P200 | -- | --
S210 | Main Harness, approximately 12 cm from Stoplamp Switch connector breakout | -- | --
S227 | Main Harness, approximately 8 cm from Stoplamp Switch connector breakout | Harness Routing Views in Wiring Systems | --
S272 | Main Harness, approximately 11 cm from G200 breakout | Harness Routing Views in Wiring Systems | --
S295 | Main Harness, approximately 7 cm from Blower Speed Selector Switch connector breakout | Harness Routing Views in Wiring Systems | --