For 1990-2009 cars

### Removal Procedure

1. Remove the child seat anchor brackets. Refer to Child Restraint Tether Anchor Replacement in Seat Belts.
2. Remove the rear floor rear trim plate (4) from the vehicle by gently disengaging the plastic retainers.

### Installation Procedure

1. Install the rear floor rear trim plate (2) to the vehicle. Ensure that the plastic retainers are completely engaged.
2. Install the child seat anchor brackets. Refer to Child Restraint Tether Anchor Replacement in Seat Belts.