For 1990-2009 cars

#### C101

Connector Part Information |

• | 097080410910

• | WHT-Main Harness

Connector Part Information

• | 097060410910

• | WHT-AC Harness

Pin | Wire Color | Function | Pin | Wire Color | Function
1 | YEL/GRN | A/C Compressor Relay Supply Voltage | 1 | YEL/GRN | A/C Compressor Relay Supply Voltage
2 | PNK | A/C Compressor Relay Control | 2 | PNK | A/C Compressor Relay Control
3 | ORN | A/C Refrigerant Pressure Signal | 3 | ORN | A/C Refrigerant Pressure Signal
4 | YEL/BLU | A/C Condensor Fan Relay Control | 4 | YEL/BLU | A/C Condensor Fan Relay Control

#### C102 (1.6L and 2.0L)

Connector Part Information |

• | 0970809nb021

• | WHT-Injector Harness

Connector Part Information

• | 0970609nb021

• | WHT-Engine Harness

Pin | Wire Color | Function | Pin | Wire Color | Function
1 | PNK | Fuel Injector 1 Control | 1 | PNK | Fuel Injector 1 Control
2 | PNK/BLK | Fuel Injector 2 Control | 2 | PNK/BLK | Fuel Injector 2 Control
3 | PNK/GRN | Fuel Injector 3 Control | 3 | PNK/GRN | Fuel Injector 3 Control
4 | PNK/BLU | Fuel Injector 4 Control | 4 | PNK/BLU | Fuel Injector 4 Control
5 | BLU/BLK | Fuel Injector Voltage Feed | 5 | BLU/BLK | Fuel Injector Voltage Feed
6 | -- | Not Used | 6 | -- | Not Used

#### C102 (2.5L)

Connector Part Information |

• | 0970509NB021

• | BLK-Fuel Injector Harness

Connector Part Information

• | 0970809NB021

• | BLK-Engine Harness

Pin | Wire Color | Function | Pin | Wire Color | Function
1 | GRY | Fuel Injector 1 | 1 | PNK | Fuel Injector 1 Control
2 | GRY/BLK | Fuel Injector 2 | 2 | PNK/BLK | Fuel Injector 2 Control
3 | GRY/WHT | Fuel Injector 3 | 3 | PNK/GRN | Fuel Injector 3 Control
4 | GRY/YEL | Fuel Injector 4 | 4 | PNK/BLU | Fuel Injector 4 Control
5 | GRY/GRN | Fuel Injector 5 | 5 | GRY/GRN | Fuel Injector 5 Control
6 | GRY/RED | Fuel Injector 6 | 6 | GRY/BLK | Fuel Injector 6 Control
7 | BLU/BLK | Fuel Injectors | 7 | BLU/BLK | Fuel Injector Voltage Feed
8--9 | -- | Not Used | 8--9 | -- | Not Used

#### C103

Connector Part Information |

• | 097080200110

• | WHT-Injector Harness

Connector Part Information

• | 097060200110

• | WHT-Main Harness

Pin | Wire Color | Function | Pin | Wire Color | Function
1 | RED | A/C FUSE Supply Voltage | 1 | RED | A/C FUSE Supply Voltage
2 | -- | Not Used | 2 | -- | Not Used

#### C200

Connector Part Information |

• | 0970520W052

• | Keyless Entry Harness

Connector Part Information

• | 0970720W0620

• | Main Harness

Pin | Wire Color | Function | Pin | Wire Color | Function
1 | BLK/ORN | Keyless Control | 1 | BLK/ORN | Keyless Control
2 | BLU | Door Lock Relay | 2 | BLU | Door Lock Relay
3 | BLU/RED | Driver Door Unlock Control | 3 | BLU/RED | Driver Door Unlock Control
4 | BLK/RED | Keyless Control | 4 | BLK/RED | Keyless Control
5 | BLK | Door Lock Relay | 5 | BLK | Door Lock Relay
6 | BLK | Door Unlock Relay | 6 | BLK | Door Unlock Relay
7 | BLK | Ground | 7 | BLK | Ground
8 | RED/WHT | Battery Positive Voltage | 8 | RED/WHT | Battery Positive Voltage
9 | RED/WHT | Battery Positive Voltage | 9 | RED/WHT | Battery Positive Voltage
10 | RED/WHT | Door Lock Relay | 10 | RED/WHT | Door Lock Relay
11 | PNK/GRN | Unlock Control | 11 | PNK/GRN | Unlock Control
12 | PNK | Lock Control | 12 | PNK | Lock Control
13 | BLU/RED | Door Unlock Relay | 13 | BLU/RED | Door Unlock Relay
14 | RED/WHT | Door Unlock Relay | 14 | RED/WHT | Door Unlock Relay
15 | BLK | Door Lock Relay | 15 | BLK | Door Lock Relay
16 | BLK | Door Unlock Relay | 16 | BLK | Door Unlock Relay
17 | PNK/WHT | Programming | 17 | PNK/WHT | Programming
18 | BLK/WHT | Ignition Positive Voltage | 18 | BLK/WHT | Ignition Positive Voltage
19 | PNK/GRN | Door Unlock Relay | 19 | PNK/GRN | Door Unlock Relay
20 | PNK | Door Lock Relay | 20 | PNK | Door Lock Relay

#### C201

Connector Part Information |

• | 0970806NB021

• | WHT-Main Harness

Connector Part Information

• | 0970720W0620

• | WHT-Main Harness

Pin | Wire Color | Function | Pin | Wire Color | Function
1-2 | -- | Not Used | 1-2 | -- | Not Used
3 | ORN/WHT | DRL Indicator Control | 3 | ORN/WHT | DRL Indicator Control
4 | -- | Not Used | 4 | -- | Not Used
5-6 | -- | Not Used | 5-6 | -- | Not Used
7 | RED/BLU | Not Used | 7 | RED/BLU | Not Used
8 | PPL | Brake Indicator Control | 8 | PPL | Brake Indicator Control
9 | PPL/GRN | Serial Data (PCM) | 9 | PPL/GRN | Serial Data (PCM)
10 | BLK/RED | Ignition Positive Voltage | 10 | BLK/RED | Ignition Positive Voltage
11-13 | -- | Not Used | 11-13 | -- | Not Used
14 | RED/GRN | Shift Indicator Lamp | 14 | RED/GRN | Shift Indicator Lamp
15 | GRY/BLU | POWER Indicator Control | 15 | GRY/BLU | POWER Indicator Control
16 | WHT/BLK | OD/OFF Indicator Control | 16 | WHT/BLK | OD/OFF Indicator Control
17 | BLU/WHT | Fuel Level Input | 17 | BLU/WHT | Fuel Level Input
18 | BLK | Ground-G200 | 18 | BLK | Ground-G200
19 | PNK/BLU | Shift Indicator | 19 | PNK/BLU | Shift Indicator
20 | GRN/BLK | Request Signal | 20 | GRN/BLK | Request Signal

#### C202

Connector Part Information |

• | 097050200510

• | WHT-IP Harness

Connector Part Information

• | 097070200510

• | WHT-Main Harness

Pin | Wire Color | Function | Pin | Wire Color | Function
1 | PNK | Blower Control High | 1 | PNK | Blower Control High
2 | BLK | Ground-G200 | 2 | BLK | Ground-G200

#### C203

Connector Part Information |

• | XNFVFS4QLIC9f

• | GRY-Main Sw. Harness

Connector Part Information

• | 0970709VB425

• | GRY-Main Harness

Pin | Wire Color | Function | Pin | Wire Color | Function
1 | YEL/BLK | Ignition Positive Voltage-ON | 1 | YEL/BLK | Ignition Positive Voltage-ON
2 | BLK | Ground-G200,G201 | 2 | BLK | Ground-G200,G201
3 | GRN | Ignition Key-In Signal | 3 | BLU/RED | Ignition Key-In Signal
4 | BLK/WHT | Ignition Positive Voltage-ON/OFF | 4 | BLK/BLU | Ignition Positive Voltage-ON/OFF
5 | BLK/YEL | Ignition Positive Voltage-Start | 5 | BLK/RED | Ignition Positive Voltage-Start
6 | BLK | Brake Indicator Control | 6 | PPL/RED | Brake Indicator Control
7 | WHT/YEL | Battery Positive Voltage | 7 | WHT/GRN | Battery Positive Voltage
8 | GRN | Battery Positive Voltage | 8 | WHT | Battery Positive Voltage
9 | BLU | Ignition Positive Voltage-ACC/ON | 9 | BLU | Ignition Positive Voltage-ACC/ON

#### C204

Connector Part Information |

• | 0970520W0623

• | BLU-Floor Harness

Connector Part Information

• | 0970720W0623

• | BLU-Main Harness

Pin | Wire Color | Function | Pin | Wire Color | Function
1 | BLK/YEL | Ground-G103 | 1 | BLK/YEL | Ground-G103
2 | GRN | Battery Positive Voltage | 2 | GRN | Battery Positive Voltage
3 | BLU/RED | Not Used | 3 | BLU/RED | Not Used
4 | BLU | Battery Positive Voltage | 4 | BLU | Battery Positive Voltage
5 | GRY/YEL | Sensor Ground | 5 | GRY/YEL | Sensor Ground
6 | RED/GRN | HO2S2 Signal | 6 | RED/GRN | HO2S2 Signal
7 | BLU/RED | Door Unlock Signal | 7 | BLU/RED | Door Unlock Signal
8 | BLU | Door Lock Signal | 8 | BLU | Door Lock Signal
9 | RED/YEL | Left Rear Window Down Signal | 9 | RED/YEL | Left Rear Window Down Signal
10 | RED/WHT | Right Rear Window Down Signal | 10 | RED/WHT | Right Rear Window Down Signal
11 | BARE | Shield Wire | 11 | BARE | Shield Wire
12 | PNK/GRN | HO2S2 Heater Control | 12 | PNK/GRN | HO2S2 Heater Control
13 | GRN/YEL | Left Rear Window Up Signal | 13 | GRN/YEL | Left Rear Window Up Signal
14 | GRN/WHT | Right Rear Window Up Signal | 14 | GRN/WHT | Right Rear Window Up Signal
15 | GRY/YEL | Sensor Ground | 15 | GRY/YEL | Sensor Ground
16 | BRN/RED | Reference Voltage | 16 | BRN/RED | Reference Voltage
17 | GRY/RED | Fuel Tank Pressure Input | 17 | GRY/RED | Fuel Tank Pressure Input
18 | -- | Not Used | 18 | -- | Not Used
19 | BLU/WHT | Ignition Positive Voltage | 19 | BLU/WHT | Ignition Positive Voltage
20 | RED/WHT | Battery Positive Voltage | 20 | RED/WHT | Battery Positive Voltage

#### C205

Connector Part Information |

• | 0970520W0620

• | WHT-Floor Harness

Connector Part Information

• | 0970720W0620

• | WHT-Main Harness

Pin | Wire Color | Function | Pin | Wire Color | Function
1 | YEL | RR Wheel Speed Sensor Signal High | 1 | YEL | RR Wheel Speed Sensor Signal High
2 | YEL/BLK | RR Wheel Speed Sensor Signal Low | 2 | YEL/BLK | RR Wheel Speed Sensor Signal Low
3 | RED | Back-Up Lamp Signal | 3 | RED | Back-Up Lamp Signal
4 | RED/BLK | Not Used | 4 | RED/BLK | Not Used
5 | LT GRN | LR Wheel Speed Sensor Signal High | 5 | LT GRN | LR Wheel Speed Sensor Signal High
6 | LT GRN/BLK | LR Wheel Speed Sensor Signal Low | 6 | LT GRN/BLK | LR Wheel Speed Sensor Signal Low
7-8 | -- | Not Used | 7-8 | -- | Not Used
9 | DK GRN/WHT | Battery Positive Voltage | 9 | DK GRN/WHT | Battery Positive Voltage
10 | RED/BLU | Not Used | 10 | RED/BLU | Not Used
11 | -- | Not Used | 11 | -- | Not Used
12 | WHT | Battery Positive Voltage | 12 | WHT | Battery Positive Voltage
13 | BLK/RED | Dome Lamp Signal | 13 | BLK/RED | Dome Lamp Signal
14 | DK GRN/RED | Not Used | 14 | DK GRN/RED | Not Used
15 | RED/BLU | Battery Positive Voltage | 15 | RED/BLU | Battery Positive voltage
16 | -- | Not Used | 16 | -- | Not Used
17 | PNK | Lock Control | 17 | PNK | Lock Control
18 | PNK/GRN | Not Used | 18 | PNK/GRN | Not Used
19 | PNK/BLK | Fuel Pump Relay Output | 19 | PNK/BLK | Fuel Pump Relay Output
20 | DK GRN/ORN | Not Used | 20 | DK GRN/ORN | Not Used

#### C206

Connector Part Information |

• | 0970522W0220

• | WHT-IP Harness

Connector Part Information

• | 0970722W0220

• | WHT-Main Harness

Pin | Wire Color | Function | Pin | Wire Color | Function
1 | BLU/ORN | ABS Indicator Control | 1 | BLU/ORN | ABS Indicator Control
2 | PPL/RED | Not Used | 2 | PPL/RED | Not Used
3 | RED/BLK | Brake Indicator | 3 | RED/BLK | Brake Indicator
4 | ORN/BLK | 4WD Indicator Control | 4 | ORN/BLK | 4WD Indicator Control
5 | YEL/BLK | Oil Pressure Indicator | 5 | YEL/BLK | Oil Pressure Indicator
6 | PNK/WHT | Programming Signal | 6 | PNK/WHT | Programming Signal
7 | ORN/BLU | Right Front Speaker (-) | 7 | ORN/BLU | Right Front Speaker (-)
8 | ORN | Right Front Speaker (+) | 8 | ORN | Right Front Speaker (+)
9 | BRN/WHT | Left Front Speaker (-) | 9 | BRN/WHT | Left Front Speaker (-)
10 | BRN/BLK | Left Front Speaker (+) | 10 | BRN/BLK | Left Front Speaker (+)
11 | PNK/WHT | Blower On Signal | 11 | PNK/WHT | Blower On Signal
12 | PNK/BLK | Blower Control Low | 12 | PNK/BLK | Blower Control Low
13 | PNK/BLU | Blower Control M1 | 13 | PNK/BLU | Blower Control M1
14 | PNK/DK GRN | Blower Control M2 | 14 | PNK/DK GRN | Blower Control M2
15 | -- | Not Used | 15 | WHT/BLK | Not Used
16 | BLU/RED | Ignition Key-In Signal | 16 | BLU/RED | Ignition Key-In Signal
17 | BLK/DK GRN | Serial Data | 17 | BLK/DK GRN | Serial Data
18 | PPL/WHT | Serial Data (EBCM) | 18 | PPL/WHT | Serial Data (EBCM)
19 | LT GRN | Mode Signal | 19 | LT GRN | Mode Signal
20 | LT GRN/WHT | Indicator Control | 20 | LT GRN/WHT | Indicator Control
21 | GRY/YEL | Cruise Indicator Control | 21 | GRY/YEL | Cruise Indicator Control
22 | PPL/YEL | MIL Control | 22 | PPL/YEL | MIL Control

#### C207

Connector Part Information |

• | 0970522W0221

• | BLK-IP Harness

Connector Part Information

• | 0970722W0221

• | BLK-Main Harness

Pin | Wire Color | Function | Pin | Wire Color | Function
1 | -- | Not Used | 1 | -- | Not Used
2 | WHT | Battery Positive Voltage | 2 | WHT | Battery Positive Voltage
3 | RED/GRN | Not Used | 3 | RED/GRN | Not Used
4 | DK GRN | Hazard Signal | 4 | DK GRN | Hazard Signal
5 | YEL | Ignition Positive Voltage | 5 | YEL | Ignition Positive Voltage
6 | RED/YEL | Lights On Signal | 6 | RED/YEL | Lights On Signal
7 | RED | HI Beam Indicator | 7 | RED | HI Beam Indicator
8 | WHT/BLU | Battery Positive Voltage | 8 | WHT/BLU | Battery Positive Voltage
9 | WHT/RED | Charge Indicator | 9 | WHT/RED | Charge Indicator
10 | -- | Not Used | 10 | -- | Not Used
11 | BLU/YEL | VSS Input | 11 | BLU/YEL | VSS Input
12 | BLK/YEL | Ground-G103 | 12 | BLK/YEL | Ground-G103
13 | YEL/WHT | ECT Sensor Input | 13 | YEL/WHT | ECT Sensor Input
14 | BRN | Engine Speed Output | 14 | BRN | Engine speed Output
15 | DK GRN/WHT | RT Outside Mirror Motor LFT/RT Control | 15 | DK GRN/WHT | RT Outside Mirror Motor LFT/RT Control
16 | LT GRN/BLK | LFT Outside Mirror Motor LFT/RT Control | 16 | LT GRN/BLK | LFT Outside Mirror Motor LFT/RT Control
17 | BRN/RED | RT Outside Mirror Motor Up/Down Control | 17 | BRN/RED | RT Outside Mirror Motor Up/Down Control
18 | BRN/YEL | LFT Outside Mirror Motor Up/Down Control | 18 | BRN/YEL | LFT Outside Mirror Motor Up/Down Control
19 | GRY | Switch Control | 19 | GRY | Switch Control
20 | BLK/RED | Idle-Up Signal | 20 | BLK/RED | Idle-Up Signal
21 | -- | Not Used | 21 | -- | Not Used
22 | YEL/DK GRN | Ignition Positive Voltage | 22 | YEL/DK GRN | Ignition Positive Voltage

#### C208

Connector Part Information |

• | 0970728W0820

• | WHT-Main Harness

Connector Part Information

• | 0970528w0820

• | WHT-Main Harness to left door

Pin | Wire Color | Function | Pin | Wire Color | Function
1 | -- | Not Used | 1 | -- | Not Used
2 | BRN/BLK | Left Front Speaker Positive | 2 | BRN/BLK | Left Front Speaker Positive
3 | -- | Not Used | 3 | -- | Not Used
4 | BRN/WHT | Left Front Speaker Negative | 4 | BRN/WHT | Left Front Speaker Negative
5 | BLU/WHT | Master Switch Battery Positive Voltage | 5 | BLU/WHT | Master Switch Battery Positive Voltage
6 | -- | Not Used | 6 | -- | Not Used
7 | GRY | Power Mirror Motor Feed Circuit | 7 | GRY | Power Mirror Motor Feed Circuit
8 | -- | Not Used | 8 | -- | Not Used
9 | DK GRN/BLK | Right Front Power Window Up Feed Circuit | 9 | DK GRN/BLK | Right Front Power Window Up Feed Circuit
10 | LT GRN/BLU | Left Power Mirror Left/Right Control Ground Circuit | 10 | LT GRN/BLU | Left Power Mirror Left/Right Control Ground Circuit
11 | BRN/YEL | Left Power Mirror Up/Down Control Ground Circuit | 11 | BRN/YEL | Left Power Mirror Up/Down Control Ground Circuit
12 | -- | Not Used | 12 | -- | Not Used
13 | RED/BLK | Right Front Window Switch Down Feed | 13 | RED/BLK | Right Front Window Switch Down Feed
14 | BLU | Door Lock Motor Voltage Feed | 14 | BLU | Door Lock Motor Voltage Feed
15 | DK GRN/WHT | Right Rear Window Switch Up Feed | 15 | DK GRN/WHT | Right Rear Window Switch Up Feed
16 | BLU/RED | Door Unlock Motor Voltage Feed | 16 | BLU/RED | Door Unlock Motor Voltage Feed
17 | DK GRN/YEL | Left Rear Window Switch Up Feed | 17 | DK GRN/YEL | Left Rear Window Switch Up Feed
18-19 | -- | Not Used | 18-19 | -- | Not Used
20 | PNK | Remote Control Door Lock Reciever Lock Control | 20 | PNK | Remote Control Door Lock Reciever Lock Control
21 | RED/YEL | Left Rear Window Switch Down Feed | 21 | RED/YEL | Left Rear Window Switch Down Feed
22-23 | -- | Not Used | 22-23 | -- | Not Used
24 | PNK/DK GRN | Remote Control Door Lock Reciever Unlock Control | 24 | PNK/DK GRN | Remote Control Door Lock Reciever Unlock Control
25 | RED/WHT | Right Rear Window Switch Down Feed | 25 | RED/WHT | Right Rear Window Switch Down Feed
26-27 | -- | Not Used | 26-27 | -- | Not Used
28 | BLK | Ground-G200 | 28 | BLK | Ground-G200

#### C209

Connector Part Information |

• | 09705065B510

• | WHT-Map Jumper Harness

Connector Part Information

• | 09707665B510

• | WHT-Main Harness

Pin | Wire Color | Function | Pin | Wire Color | Function
1 | -- | Not Used | 1 | -- | Not Used
2 | WHT | Battery Positive Voltage | 2 | WHT | Battery Positive Voltage
3 | BLK/RED | Door Lock Signal | 3 | BLK/RED | Door Lock Signal
4 | BLK | Ground-G200 | 4 | BLK | Ground-G200
5-6 | BARE | Not Used | 5-6 | BARE | Not Used

#### C210-California Only

Connector Part Information |

• | 0970706VB020

• | WHT-Main Harness

Connector Part Information

• | 0970506VB020

• | WHT-Main Harness

Pin | Wire Color | Function | Pin | Wire Color | Function
1 | GRY/YEL | HO2S Sensor Ground | 1 | GRY/YEL | HO2S Sensor Ground
2 | RED/GRN | HO2S 5 volt reference signal | 2 | RED/GRN | HO2S 5 volt reference signal
3-4 | -- | Not Used | 3-4 | -- | Not Used
5 | -- | Shield | 5 | -- | Shield
6 | PNK/GRN | HO2S Heater Control | 6 | PNK/GRN | HO2S Heater Control

#### C211

Connector Part Information |

• | 0970728W0820

• | WHT-Main Harness

Connector Part Information

• | 0970528W082

• | WHT-Door Harness

Pin | Wire Color | Function | Pin | Wire Color | Function
1 | -- | Not Used | 1 | -- | Not Used
2 | ORN | Right Front Speaker Positive | 2 | ORN | Right Front Speaker Positive
3 | -- | Not Used | 3 | -- | Not Used
4 | ORN/BLU | Right Front Speaker Negative | 4 | ORN/BLU | Right Front Speaker Negative
5 | BLU/WHT | Master Window Switch Battery Positive Voltage | 5 | BLU/WHT | Master Window Switch Battery Positive Voltage
6 | -- | Not Used | 6 | -- | Not Used
7 | GRY | Power Mirror Supply Voltage | 7 | GRY | Power Mirror Supply Voltage
8 | -- | Not Used | 8 | -- | Not Used
9 | GRN/BLK | Right Front Window Switch Up Voltage Feed. | 9 | GRN/BLK | Right Front Window Switch Up Voltage Feed.
10 | GRN/WHT | Right Power Mirror Left/Right Voltage Feed | 10 | GRN/WHT | Right Power Mirror Left/Right Voltage Feed
11 | BRN/RED | Right Power Mirror Up/Down Voltage Feed | 11 | BRN/RED | Right Power Mirror Up/Down Voltage Feed
12 | -- | Not Used | 12 | -- | Not Used
13 | RED/BLK | Right Front Window Switch Down Voltage Feed | 13 | RED/BLK | Right Front Window Switch Down Voltage Feed
14 | BLU | Door Lock Motor Supply Voltage | 14 | BLU | Door Lock Motor Supply Voltage
15 | -- | Not Used | 15 | -- | Not Used
16 | BLU/RED | Door Unlock Motor Supply Voltage | 16 | BLU/RED | Door Unlock Motor Supply Voltage
17-19 | -- | Not Used | 17-19 | -- | Not Used
20 | PNK | Remote Control Door Lock Reciever Lock Control | 20 | PNK | Remote Control Door Lock Reciever Lock Control
21-27 | -- | Not Used | 21-27 | -- | Not Used
28 | BLK | Ground-G201 | 28 | BLK | Ground-G201

#### C212

Connector Part Information |

• | 0970524WB121

• | BLK-Engine Harness 2.0

Connector Part Information

• | 0970724WB121

• | BLK-Main Harness

Pin | Wire Color | Function | Pin | Wire Color | Function
1 | YEL/WHT | ECT Gage | 1 | YEL/WHT | ECT Gage
2 | BLU/YEL | VSS Input | 2 | BLU/YEL | VSS Input
3 | ORN/GRN | Relay Control | 3 | ORN/GRN | Relay Control
4 | BLK/GRN | Shield Wire | 4 | -- | Shield Wire
5 | -- | Not Used | 5 | -- | Not Used
6 | RED | Axle Actuator Control | 6 | RED | Axle Actuator Control
7-8 | -- | Not Used | 7-8 | -- | Not Used
9 | GRY/YEL | Sensor Ground | 9 | GRY/YEL | Sensor Ground
10 | BLK | Ground-G201 | 10 | BLK | Ground-G201
11 | BLU/BLK | Main Relay Output | 11 | BLU/BLK | Main Relay Output
12 | RED | Back-Up Lamp Signal | 12 | RED | Back-Up Lamp Signal
13-15 | -- | Not Used | 13-15 | -- | Not Used
16 | BLK/YEL | Ground-G103 | 16 | BLK/YEL | Ground-G103
17 | YEL/BLK | Oil Pressure Indicator | 17 | YEL/BLK | Oil Pressure Indicator
18 | PNK | Axle Actuator Control | 18 | PNK | Axle Actuator Control
19 | BLK/YEL | Start Signal M/T | 19 | BLK/YEL | Start Signal M/T
20 | BLK/RED | Ignition Positive Voltage A/T | 20 | BLK/RED | Ignition Positive Voltage A/T
21 | BLK/GRN | DLC Ground | 21 | BLK/GRN | DLC Ground
22 | BLK/WHT | Ignition Positive Voltage | 22 | BLK/WHT | Ignition Positive Voltage
23 | YEL | Ignition Positive Voltage | 23 | YEL | Ignition Positive Voltage
24 | WHT/RED | Charge Indicator | 24 | WHT/RED | Charge Indicator

#### C213

Connector Part Information |

• | 0970520W0621

• | BLK-IP Harness

Connector Part Information

• | 0970720w0621

• | BLK-Floor Harness

Pin | Wire Color | Function | Pin | Wire Color | Function
1 | DK GRN/BLU | Not Used | 1 | DK GRN/BLU | Not Used
2 | RED/YEL | Battery Positive Voltage | 2 | RED/YEL | Battery Positive Voltage
3 | BLU/WHT | Fuel Level Input | 3 | BLU/WHT | Fuel Level Input
4 | -- | Not Used | 4 | -- | Not Used
5 | ORN | Ignition Positive Voltage | 5 | ORN | Ignition Positive Voltage
6 | -- | Not Used | 6 | -- | Not Used
7 | LT GRN | Left Rear Speaker (+) | 7 | LT GRN | Left Rear Speaker (+)
8 | GRY | Right Rear Speaker (+) | 8 | GRY | Right Rear Speaker (+)
9 | GRY/RED | Seat Belt Indicator | 9 | GRY/RED | Seat Belt Indicator
10 | -- | Not Used | 10 | -- | Not Used
11 | BLK/BLU | Door Open Signal | 11 | BLK/BLU | Door Open Signal
12 | -- | Not Used | 12 | -- | Not Used
13 | BLK/RED | Not Used | 13 | BLK/RED | Not Used
14 | -- | Not Used | 14 | -- | Not Used
15 | BLU | Ignition Positive Voltage | 15 | BLU | Ignition Positive Voltage
16 | -- | Not Used | 16 | -- | Not Used
17 | LT GRN/BLK | Left Rear Speaker (-) | 17 | LT GRN/BLK | Left Rear Speaker (-)
18 | GRY/BLK | Right Rear Speaker (-) | 18 | GRY/BLK | Right Rear Speaker (-)
19 | BLK/RED | Relay Control | 19 | BLK/RED | Relay Control
20 | -- | Not Used | 20 | -- | Not Used

#### C214

Connector Part Information |

• | 097050810010

• | WHT-Main Harness

Connector Part Information

• | 097070810010

• | WHT-A/C Jumper Harness

Pin | Wire Color | Function | Pin | Wire Color | Function
1 | PNK/WHT | Idle-UP Control | 1 | PNK/WHT | Idle-Up Control
2 | PNK | A/C Compressor Relay Control | 2 | PNK | A/C Compressor Relay Control
3 | GRN/BLK | Request Signal | 3 | GRN/WHT | Request Signal
4 | BLK/YEL | Ground-G103 | 4 | BLK | Ground-G103
5 | YEL/BLK | A/C Idle-Up | 5 | YEL/BLK | A/C Idle-Up
6 | BLK/WHT | Ignition Positive Voltage | 6 | BLK/WHT | Ignition Positive Voltage
7 | GRY/WHT | A/C Cut-Out | 7 | GRN/YEL | A/C Cut-Out
8 | ORN | A/C Refrigerant Pressure Signal | 8 | ORN | A/C Refrigerant Pressure Signal

#### C215

Connector Part Information |

• | 0970505W0122

• | YEL

Connector Part Information

• | 0970705W0122

• | YEL

Pin | Wire Color | Function | Pin | Wire Color | Function
1 | YEL/GRN | Air Bag Warning Control | 1 | BLU | Air Bag Warning Control
2 | BLK | Ground-G200 | 2 | -- | Not Used
3 | -- | Not Used | 3 | -- | Not Used
4 | GRY/RED | Seat Belt Switch Signal | 4 | YEL/BLU | Seat Belt Switch Signal
5 | PPL/GRN | Serial Data | 5 | WHT/BLK | Serial Data

#### C301

Connector Part Information |

• | 097060210220

• | WHT

Connector Part Information

• | 0970802102

• | WHT

Pin | Wire Color | Function | Pin | Wire Color | Function
1 | BLU | Battery Positive Voltage | 1 | BLU | Battery Positive Voltage
2 | BLU/RED | Ground-G201 | 2 | BLU/RED | Ground-G201

#### C302

Connector Part Information |

• | 097080310720

• | WHT

Connector Part Information

• | 097060310620

• | WHT

Pin | Wire Color | Function | Pin | Wire Color | Function
--- | --- | --- | --- | --- | ---
1 | BLU/WHT | Door Lock Switch Voltage Supply | 1 | BLU/WHT | Door Lock Switch Voltage Supply
2 | GRN/YEL | Left Rear Window Switch Up Feed | 2 | GRN/YEL | Left Rear Window Switch Up Feed
3 | RED/YEL | Left Rear Window Switch Down Feed | 3 | RED/YEL | Left Rear Window Switch Down Feed

#### C303

Connector Part Information |

• | 097060210220

• | WHT

Connector Part Information

• | 0970802102

• | WHT

Pin | Wire Color | Function | Pin | Wire Color | Function
1 | BLU | Battery Positive Voltage | 1 | BLU | Battery Positive Voltage
2 | BLU/RED | Ground-G201 | 2 | BLU/RED | Ground-G201

#### C304

Connector Part Information |

• | 097080310720

• | WHT

Connector Part Information

• | 097060310620

• | WHT

Pin | Wire Color | Function | Pin | Wire Color | Function
--- | --- | --- | --- | --- | ---
1 | BLU/WHT | Door Lock Switch Voltage Supply | 1 | BLU/WHT | Door Lock Switch Voltage Supply
2 | GRN/YEL | Left Rear Window Switch Up Feed | 2 | GRN/YEL | Left Rear Window Switch Up Feed
3 | RED/YEL | Left Rear Window Switch Down Feed | 3 | RED/YEL | Left Rear Window Switch Down Feed

#### C305

Connector Part Information |

• | 097070610410

• | WHT

Connector Part Information

• | 097060310620

• | WHT

Pin | Wire Color | Function | Pin | Wire Color | Function
1 | GRN/YEL | Left Rear Window Switch Up Feed | 1 | GRN/YEL | Left Rear Window Switch Up Feed
2 | BLU/WHT | Door Lock Switch Voltage Supply | 2 | BLU/WHT | Door Lock Switch Voltage Supply
3 | BLU/RED | Left Rear Door Unlock Motor Feed | 3 | BLU/RED | Left Rear Door Unlock Motor Feed
4 | RED/YEL | Left Rear Window Switch Down Feed | 4 | RED/YEL | Left Rear Window Switch Down Feed
5 | -- | Not Used | 5 | -- | Not Used
6 | BLU | Left Rear Door Lock Motor Feed | 6 | BLU | Left Rear Door Lock Motor Feed

#### C400

Connector Part Information |

• | 097051310110

• | NAT-Back Door Harness

Connector Part Information

• | 097071310110

• | NAT-Floor Harness

Pin | Wire Color | Function | Pin | Wire Color | Function
1 | ORN | Rear Wiper OFF Signal | 1 | ORN | Rear Wiper OFF Signal
2 | PNK | Lock Control | 2 | PNK | Lock Control
3 | BLK/RED | Relay Control | 3 | BLK/RED | Relay Control
4 | YEL/BLU | Ignition Positive Voltage | 4 | YEL/BLU | Ignition Positive Voltage
5 | RED/WHT | Ignition Positive Voltage | 5 | RED/WHT | Ignition Positive Voltage
6 | BLU | Door Lock Relay Control | 6 | BLU | Door Lock Relay Control
7 | GRN/WHT | Battery Positive Voltage | 7 | GRN/WHT | Battery Positive Voltage
8 | -- | Not Used | 8 | YEL/BLU | Not Used
9 | RED/YEL | Battery Positive Voltage | 9 | RED/YEL | Battery Positive Voltage
10 | BLU/GRN | Rear Washer OFF Signal | 10 | BLU/GRN | Rear Washer OFF Signal
11 | BLU/RED | Door Unlock Relay Control | 11 | BLU/RED | Door Unlock Relay Control
12 | -- | Not Used | 12 | -- | Not Used
13 | BLK | Ground-G401 | 13 | BLK | Ground-G400

#### C401

Connector Part Information |

• | 0970612NB021

• | BLK-Fuel Jumper Harness

Connector Part Information

• | 0970812NB021

• | BLK-Floor Harness

Pin | Wire Color | Function | Pin | Wire Color | Function
1 | BLK | Ground-G400 | 1 | BLK | Ground-G400
2 | PNK/BLK | Fuel Pump Relay Output | 2 | PNK/BLK | Fuel Pump Relay Output
3 | BLK/YEL | Ground-G103 | 3 | BLK/YEL | Ground-G103
4 | BLU/WHT | Fuel Level Input | 4 | BLU/WHT | Fuel Level Input
5 | -- | Not Used | 5 | -- | Not Used
6 | BRN/RED | Reference Voltage | 6 | BRN/RED | Reference Voltage
7 | GRY/YEL | Sensor Ground | 7 | GRY/YEL | Sensor Ground
8 | GRY/RED | Fuel Tank Pressure Input | 8 | GRY/RED | Fuel Tank Pressure Input
9 | YEL | RT Rear Wheel Speed Sensor Signal High | 9 | YEL | RT Rear Wheel Speed Sensor High
10 | YEL/BLK | RT Rear Wheel Speed Sensor Low | 10 | YEL/BLK | RT Rear Wheel Speed Sensor Low
11 | LT GRN | LFT Rear Wheel Speed Sensor High | 11 | LT GRN | LFT Rear Wheel Speed Sensor High
12 | LT GRN/BLK | LFT Rear Wheel Speed Sensor Low | 12 | LT GRN/BLK | LFT Rear Wheel Speed Sensor Low

#### C403

Connector Part Information |

• | 097050210210

• | NAT-Floor Harness

Connector Part Information

• | 097070210310

• | NAT-Back Door Harness

Pin | Wire Color | Function | Pin | Wire Color | Function
1 | GRN/WHT | Battery Positive Voltage | 1 | GRN/WHT | Battery Positive Voltage
2 | BLK | Ground, G401 | 2 | BLK | Ground, G401