For 1990-2009 cars

### Removal Procedure

1. Remove the front wiper arms. Refer to Windshield Wiper Arm Replacement in Wipers/Washer Systems.
2. Remove the following components from the vehicle:

2.1. | The 8 plastic retainers

2.2. | The air inlet screen (1)

### Installation Procedure

1. Install the air inlet screen (1) to the vehicle. Secure the screen with 8 plastic retainers.
2. Install the front wiper arms. Refer to Windshield Wiper Arm Replacement in Wipers/Washer Systems.