For 1990-2009 cars

### Removal Procedure

1. Remove the front floor console. Refer to Console Replacement in Instrument Panel, Gauges, and Console.
2. Gently pry the power window switch out of the console.

### Installation Procedure

1. Install the power window switch by snapping the power window switch into the front floor console.
2. Install the front floor console. Refer to Console Replacement in Instrument Panel, Gauges, and Console.