For 1990-2009 cars

### Removal Procedure

1. Remove the rear security cover. Refer to Security Panel Replacement .
2. Unattach the 2 loops that retain the rear compartment convenience net (3) to each of the rear security cover hook and brackets (1).
3. Remove the rear compartment convenience net (3) from the vehicle.

### Installation Procedure

1. Install the rear compartment convenience net (3) to the vehicle. Secure the net by attaching each of the loops to the respective hook and bracket (1).
2. Install the rear security cover. Refer to Security Panel Replacement .