For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Fuse Block 2 | Under the LH instrument panel | Power and Grounding Component Views in Wiring Systems | --
Rear Defogger (4-Door) | In the rear window | -- | --
Rear Defogger Switch (4-Door) | LH instrument panel to the left of the steering column | -- | --
C200 (22 Cavities) | Main harness to the instrument panel harness, LH instrument panel near fuse block 2 | Harness Routing Views in Wiring Systems | --
C201 (16 Cavities) | Main harness to the instrument panel harness, LH instrument panel near fuse block 2 | Harness Routing Views in Wiring Systems | --
C211 (16 Cavities) | Instrument panel harness to the floor harness, RH instrument panel near the A-pillar | Harness Routing Views in Wiring Systems | --
C400 (12 Cavities) | Floor harness to the rear lamp harness behind the LH rear wheelhousing | Harness Routing Views in Wiring Systems | --
C410 (1 Cavity) (4-Door) | Rear lamp harness to the rear door harness behind the RH rear wheelhousing | Harness Routing Views in Wiring Systems | --
G200 | Behind the LH instrument panel above fuse block 2 | Power and Grounding Component Views in Wiring Systems | --
G400 (4-Door) | Inside the rear door near the license plate lamps | Power and Grounding Component Views in Wiring Systems | --
G400 (2-Door) | Inside the rear door near the license plate lamps | Power and Grounding Component Views in Wiring Systems | --
P400 (2-Door) | Rear door | Power and Grounding Component Views in Wiring Systems | --
P400 (4-Door) | Rear door | Power and Grounding Component Views in Wiring Systems | --
P401 | Rear of the vehicle to the right of the LH frame rail | Power and Grounding Component Views in Wiring Systems | --
P402 | Rear of the vehicle to the left of the RH frame rail | Power and Grounding Component Views in Wiring Systems | --
S225 | Instrument panel harness approximately 12 cm (4.72 in) from the cigar lighter | Harness Routing Views in Wiring Systems | --
S226 | Instrument panel harness approximately at the radio breakout | Harness Routing Views in Wiring Systems | --
S230 | Main harness approximately 5 cm (1.96 in) from the G300 breakout | Harness Routing Views in Wiring Systems | --
S235 | Instrument panel harness approximately 1 cm (0.39 in) from the C211 breakout | Harness Routing Views in Wiring Systems | --
S262 | Main harness approximately 8 cm (3.14 in) from the stoplamp switch connector breakout | Harness Routing Views in Wiring Systems | --
S278 (with ABS) | Main harness approximately 14 cm (5.51 in) from the G200 breakout | Harness Routing Views in Wiring Systems | --
S400 | Rear door harness near G400 breakout | Harness Routing Views in Wiring Systems | --