For 1990-2009 cars

## Instrument Panel Accessory Trim Plate Replacement Center

### Removal Procedure

1. Remove the ashtray from the guide by depressing the spring-loaded tab and pulling the ashtray rearward.
2. Remove the following components from the instrument panel:

2.1. | The 3 screws (2)

2.2. | The IP accessory center trim plate (1)

### Installation Procedure

1. Install the IP accessory center trim plate (1) to the instrument panel. Secure the plate with 3 screws (2).
2. Slide the ashtray into the guide.