For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 |

1. Set the dome lamp to the DOOR position.
2. Open and close the left front door.

The front dome lamps will remain on 15-20 seconds each time the door is closed.

The rear lamp will turn on and off each time the door is open and closed.

--

2 | Turn the dome lamp to the ON position and then back to the DOOR position. | The dome lamp lights, then goes out. | --
3 |

1. Turn the dome lamp to the OFF position.
2. Open and Close the left front door.

The dome lamp does not light at all.

--

4 | Open and close the back door. | The rear compartment lamp lights when the back door is open. The lamp goes out when the back door is closed. | --
* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.