For 1990-2009 cars

### Removal Procedure

1. Remove the illumination lamp bulb socket from the cigar lighter.
2. Disconnect the cigar lighter electrical connector.
3. Remove the cigar lighter bulb socket from the lamp.
4. Remove the bulb from the cigar lighter bulb socket.

### Installation Procedure

1. Install the bulb to the cigar lighter bulb socket.
2. Install the cigar lighter bulb socket to the lamp.
3. Connect the cigar lighter electrical connector.
4. Install the illumination bulb socket to the cigar lighter.