For 1990-2009 cars

Component | Metric | English
--- | --- | ---
Accumulator Pistons and Springs

- Direct Clutch Accumulator Piston Outer Diameter

31.80-31.85

1.252-1.254

- Direct Clutch Accumulator Piston Upper Spring Free Length

42.35

1.667

- Forward Clutch Accumulator Piston Lower Spring Free Length

29.50

1.161

- Forward Clutch Accumulator Piston Outer Diameter

31.80-31.85

1.252-1.254

- Forward Clutch Accumulator Piston Upper Spring Free Length

57.18

2.251

- Second Brake Accumulator Piston Lower Spring Free Length

35.13

1.383

- Second Brake Accumulator Piston Outer Diameter

34.80-34.85

1.370-1.372

- Second Brake Accumulator Piston Upper Spring Free Length

55.18

2.172

Front Upper Valve Body Springs

- Cut Back Valve Spring Coil Outer Diameter

6.85

0.269

- Cut Back Valve Spring Free Length

23.00

0.905

- Secondary Regulator Valve Spring Coil Outer Diameter

17.43

0.681

- Secondary Regulator Valve Spring Free Length

71.23

2.804

- Secondary Valve Spring Coil Outer Diameter

8.58

0.337

- Secondary Valve Spring Free Length

19.24

0.757

- Throttle Valve Primary Spring Coil Outer Diameter

10.90

0.429

- Throttle Valve Primary Spring Free Length

39.55

1.557

Lower Valve Body Springs

- Ball Valve Spring Coil Outer Diameter

11.11

0.437

- Ball Valve Spring Free Length

32.14

1.265

- Bypass Valve Spring Coil Outer Diameter

13.82

0.554

- Bypass Valve Spring Free Length

33.32

1.312

- Inter Coast Modulator Valve Spring Coil Outer Diameter

10.00

0.394

- Inter Coast Modulator Valve Spring Free Length

35.43

1.395

- Low Coast Modulator Valve Spring Coil Outer Diameter

10.00

0.394

- Low Coast Modulator Valve Spring Free Length

42.35

1.667

- Pressure Relief Valve Spring Free Length

38.14

0.501

- Pressure Relief Valve Spring Coil Outer Diameter

13.14

0.517

- Primary Regulator Valve Spring Coil Outer Diameter

17.20

0.677

- Primary Regulator Valve Spring Free Length

56.30

2.216

- TCC Lock-Up Control Valve Spring Coil Outer Diameter

11.30

0.445

- TCC Lock-Up Control Valve Spring Free Length

34.60

1.362

- Valve Damping Spring Coil Outer Diameter

4.95

0.195

- Valve Damping Spring Free Length

20.00

0.787

Rear Upper Valve Body Springs

- Reverse Brake Sequence Valve Spring Coil Outer Diameter

9.20

0.362

- Reverse Brake Sequence Valve Spring Free Length

37.55

1.148

- 1-2 Shift Valve Coil Spring Outer Diameter

8.90

0.350

- 1-2 Shift Valve Spring Free Length

29.15

1.147

- 2-3 Shift Valve Spring Coil Outer Diameter

8.90

0.350

- 2-3 Shift Valve Spring Free Length

29.15

1.147

- 3-4 Shift Valve Spring Coil Outer Diameter

8.90

0.350

- 3-4 Shift Valve Spring Free Length

29.15

1.147

Transmissions

- B1 Brake Piston Stroke

0.63-1.73

0.025-0.068

- B2 Brake Piston Stroke

1.01-2.25

0.040-0.088

- Direct Clutch Piston Return Spring Free Length

15.13

0.594

- Direct Clutch Piston Stroke

0.19-1.75

0.008-0.068

- Forward Clutch Piston Return Spring Free Length

15.10

0.595

- Forward Clutch Piston Stroke

1.40-2.24

0.056-0.880

- Oil Pump Body-to-Driven Gear Clearance

0.07-0.15

0.0028-0.0059

- Oil Pump Drive Gear and Driven Gear Side Clearance

0.02-0.05

0.0008-0.0019

- Oil Pump Drive Gear Tip Clearance

0.11-0.14

0.0044-0.0055

- Output Shaft End Play

0.30-0.90

0.012-0.035

- Overdrive (Case Side) Clutch Piston Return Springs Free Length

15.10

0.594

- Overdrive (Case Side) Snap Ring-to-Brake Flange Clearance

0.35-1.91

0.014-0.075

- Overdrive (Planetary Gear Side) Clearance

1.47-2.28

0.058-0.089

Component | Specification
--- | ---
Metric | English

- B1 Brake Piston Stroke

0.63-1.73 mm

0.025-0.068 in

- B2 Brake Piston Stroke

1.01-2.25 mm

0.040-0.088 in

- Direct Clutch Piston Return Spring Free Length

15.13 mm

0.594 in

- Direct Clutch Piston Stroke

0.19-1.75 mm

0.008-0.068 in

- Forward Clutch Piston Return Spring Free Length

15.10 mm

0.595 in

- Forward Clutch Piston Stroke

1.40-2.24 mm

0.056-0.880 in

- Oil Pump Body-to-Driven Gear Clearance

0.07-0.15 mm

0.0028-0.0059 in

- Oil Pump Drive Gear and Driven Gear Side Clearance

0.02-0.05 mm

0.0008-0.0019 in

- Oil Pump Drive Gear Tip Clearance

0.11-0.14 mm

0.0044-0.0055 in

- Output Shaft End Play

0.30-0.90 mm

0.012-0.035 in

- Overdrive (Case Side) Clutch Piston Return Springs Free Length

15.10 mm

0.594 in

- Overdrive (Case Side) Snap Ring-to-Brake Flange Clearance

0.35-1.91 mm

0.014-0.075 in

- Overdrive (Planetary Gear Side) Clearance

1.47-2.28 mm

0.058-0.089 in