For 1990-2009 cars

System | DTCs Required to Set System Status to YES
--- | ---
Catalyst | DTC P0420 or P0430 Catalyst System Low Efficiency
EVAP | DTC P0440 Evaporative Emission (EVAP) System DTC P0455 Evaporative Emission (EVAP) System Leak
Oxygen Sensor | DTC P0131 or P0151 HO2S Circuit Low Voltage Sensor 1 DTC P0132 or P0152 HO2S Circuit High Voltage Sensor 1 DTC P0133 or P0153 HO2S Slow Response Sensor 1 DTC P0134 or P0154 HO2S Insufficient Activity Sensor 1 DTC P0136 or P0156 HO2S Circuit Sensor 2
Oxygen Sensor Heater | DTC P0135 or P0155 Heater Performance Sensor 1 DTC P0141 Heater Performance Bank 1 Sensor 2 DTC P0161 Heater Performance Bank 2 Sensor 2