For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Synchronizer Ring-to-Gear Clearance (Maximum) | 1.0-1.4 mm | 0.039-0.055 in
Synchronizer Ring Key Slot Width (Maximum) | 10.1-10.4 mm | 0.397-0.409 in
Gear Shift Fork-to-Synchronizer Sleeve Clearance (Maximum) | 1.0 mm | 0.039 in
Locating Spring Length (Standard Length) | 24.0-27.0 mm | 0.945-1.063 in
Locating Spring Length (Service Limit) | 24.0 mm | 0.945 in

#### Manual Transmission Drain and Refill

Application | Specification
--- | ---
Metric | English
Two-Wheel Drive | 1.9 liters | 2.0 quarts
Four-Wheel Drive | 1.5 liters | 1.6 quarts
Oil Recommended | 75W-90 GL4 Lubricant or equivalent