For 1990-2009 cars

## Power Steering Pump Description 1.6L

The power steering pump is a vane-type pump. The drive belt, coming from the crankshaft pulley, drives the power steering pump.

As the discharge rate of the power steering pump increases in proportion to the pump revolution speed, the power steering fluid pressure increases. The flow control valve controls the maximum amount of fluid pressure necessary for the steering operation.

#### Power Steering Pump -- Disassembled View

(1) | Power Steering Pump Pulley
(2) | Power Steering Pump Seal
(3) | Idle Speed Control Power Steering Pressure Switch
(4) | Power Steering Pump Body
(5) | Power Steering Pump Seal
(5) | Power Steering Pump Seal
(5) | Power Steering Pump Seal
(5) | Power Steering Pump Seal
(6) | Power Steering Pump Side Plate
(7) | Power Steering Pump Vane
(8) | Power Steering Pump Rotor
(9) | Snap Ring
(10) | Power Steering Pump Cam Ring
(11) | Power Steering Pump Cover
(12) | Flow Control Valve Plug
(13) | Flow Control Valve Spring
(14) | Flow Control Valve (Relief Valve)
(15) | Flow Control Valve Assembly
(16) | Power Steering Pump Inlet Hose Connector

## Power Steering Pump Description 2.0L

The power steering pump is a vane-type pump. The drive belt, coming from the crankshaft pulley, drives the power steering pump.

As the discharge rate of the power steering pump increases in proportion to the pump revolution speed, the power steering fluid pressure increases. The flow control valve controls the maximum amount of fluid pressure necessary for the steering operation.

#### Power Steering Pump -- Disassembled View

(1) | Power Steering Pump Inlet Hose Connector
(2) | Power Steering Pump Seal
(3) | Power Steering Pump Cover
(4) | Power Steering Pump Seal
(5) | Power Steering Pump Side Plate and Rotor
(6) | Power Steering Pump Seal
(7) | Power Steering Pump Seal
(8) | Power Steering Pump Body
(9) | Power Steering Pump Pulley
(10) | Idle Speed Control Power Steering Pressure Switch
(11) | Power Steering Pump Seal