For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
A/C Compressor Control Module | Behind the RH instrument panel on the evaporator | HVAC Component Views in HVAC Manual with A/C | HVAC Connector End Views in HVAC Manual with A/C
A/C Compressor Clutch | LH front engine compartment attached to the A/C compressor | HVAC Component Views in HVAC Manual with A/C | --
A/C Compressor Clutch Relay | RH engine compartment near fuse block 1 | HVAC Component Views in HVAC Manual with A/C | HVAC Connector End Views in HVAC Manual with A/C
A/C Condenser Fan | Between the grille and the radiator | HVAC Component Views in HVAC Manual with A/C | --
A/C Condenser Fan Relay | RH engine compartment near fuse block 1 | HVAC Component Views in HVAC Manual with A/C | HVAC Connector End Views in HVAC Manual with A/C
A/C Switch | Center of the instrument panel above the radio | -- | --
Blower Speed Selector Switch | Center of the instrument panel above the radio | HVAC Component Views in HVAC Manual Non-A/C | HVAC Connector End Views in HVAC Manual Non-A/C
Refrigerant Pressure Switch | RH front engine compartment behind the radiator | HVAC Component Views in HVAC Manual Non-A/C | --
Engine Coolant Temperature (ECT) Sensor | RH side of the engine in the thermostat housing | Engine Controls Component Views in Engine Controls-1.6L | --
Evaporator Temperature Sensor | Behind the RH instrument panel in the evaporator housing | -- | --
Fuse Block 1 | RH engine compartment in front of the battery | Power and Grounding Component Views in Wiring Systems | --
C2 (1 Cavities) | A/C harness to fuse block 1 below fuse block 1 | Power and Grounding Component Views in Wiring Systems | --
Fuse Block 2 | Under the LH instrument panel | Power and Grounding Component Views in Wiring Systems | --
Powertrain Control Module (PCM) | Under the LH instrument panel to the left of the steering column | Engine Controls Component Views in Engine Controls-1.6L | Powertrain Control Module Connector End Views in Engine Controls
3-Speed Automatic and Manual Transmissions C1 (22 Cavities) | Main harness to the PCM, behind the instrument panel to the left of the steering column | -- | --
4-Speed Automatic and Manual Transmissions C1 (22 Cavities) | Main harness to the PCM, behind the instrument panel to the left of the steering column | -- | --
C108 (4 Cavities) | Main harness to the A/C sub-harness behind the RH headlamp | Harness Routing Views in Wiring Systems | --
C212 (10 Cavities) | Main harness to the A/C compressor control module jumper harness, RH instrument panel behind the instrument panel compartment | Harness Routing Views in Wiring Systems | --
C217 (6 Cavities) | Main harness to the blower speed selector switch, RH instrument panel | Harness Routing Views in Wiring Systems | --
G108 (with A/C) | RH inner fender near the battery | Power and Grounding Component Views in Wiring Systems | --
G202 | Behind the center instrument panel on the bulkhead | Power and Grounding Component Views in Wiring Systems | --
P200 | LH rear engine compartment on the bulkhead near the brake master cylinder | Power and Grounding Component Views in Wiring Systems | --
P201 | RH rear engine compartment on the bulkhead near the battery | Power and Grounding Component Views in Wiring Systems | --
S110 | Outer A/C harness RH engine compartment near the strut tower | Harness Routing Views in Wiring Systems | --
S114 | Outer A/C harness RH engine compartment near the strut tower | Harness Routing Views in Wiring Systems | --
S131 | Main harness approximately 19 cm from P201 | Harness Routing Views in Wiring Systems | --
S209 | Main harness approximately 12 cm from the blower speed selector switch connector breakout | Harness Routing Views in Wiring Systems | --
S220 | Main harness approximately 1 cm from the blower speed selector switch connector breakout | Harness Routing Views in Wiring Systems | --