For 1990-2009 cars

#### Fuse Block C1

Connector Part Information |

• | 097050302521

• | BLK

Pin | Wire Color | Function
--- | --- | ---
1 | BLK/RED | FI Fuse 15A
2 | WHT/RED | H/L,R Fuse 15A
3 | WHT/BLU | H/L,L Fuse 15A

#### Fuse Block C4

Connector Part Information |

• | 097050290521

• | BLK

Pin | Wire Color | Function
--- | --- | ---
1 | WHT/GRN | LAMP Fuse 30A
2 | WHT/YEL | IG Fuse 60A

#### Junction Block C1

Connector Part Information |

• | 0970511W0220

• | WHT

Pin | Wire Color | Function
--- | --- | ---
1 | -- | Not Used
2 | RED/YEL | Tail Relay Output
3 | BLU/WHT | Ignition Positive Voltage-P/W Fuse 30A
4 | YEL | Ignition Positive Voltage-TURN Fuse 10A
5 | -- | Not Used
6 | BLK | Ground-G200, G201
7-8 | -- | Not Used
9 | WHT | Battery Positive Voltage-DOME Fuse 10A
10 | GRN | Battery Positive Voltage-STOP Fuse 15A
11 | RED/WHT | Battery Positive Voltage-D/L Fuse 20A

#### Junction Block C2

Connector Part Information |

• | 097050460020

• | WHT

Pin | Wire Color | Function
--- | --- | ---
1 | BLK/BLU | Ignition Positive Voltage
2 | BLU | Ignition Positive Voltage
3 | YEL/BLK | Ignition Positive Voltage
4 | WHT/YEL | Battery Positive Voltage

#### Junction Block C3

Connector Part Information |

• | 0970510W0340

• | WHT

Pin | Wire Color | Function
--- | --- | ---
1 | GRN/YEL | Right Turn Signal
2 | GRN/YEL | Right Turn Signal
3 | BLK/WHT | Ignition Positive Voltage-IG Fuse 20A
4 | -- | Not Used
5 | GRN/RED | Left Turn Signal
6 | GRN/RED | Left Turn Signal
7 | -- | Not Used
8 | YEL/BLU | Ignition Positive Voltage-WIP Fuse 15A
9 | GRN | Turn/Hazard Flasher Output
10 | -- | Not Used

#### Junction Block C4

Connector Part Information |

• | 0970511w0320

• | WHT

Pin | Wire Color | Function
--- | --- | ---
1 | BLK/WHT | IG Fuse
2 | WHT/BLK | CIG Fuse 20A
3 | YEL/GRN | DEF Fuse 15A
4 | YEL/RED | Turn/Hazard Flasher
5 | YEL/BLU | WIP Fuse 15A
6 | -- | Not Used
7 | GRN/YEL | Hazard Switch RH Turn Lamp
8 | WHT/GRN | HAZ Fuse 15A
9 | GRN/RED | Hazard Switch LH Turn Lamp
10 | -- | Not Used
11 | RED/GRN | TAIL Fuse 15A

#### Junction Block C5

Connector Part Information |

• | 0970506W0240

• | WHT

Pin | Wire Color | Function
--- | --- | ---
1 | -- | Not Used
2 | BLK/WHT | Ignition Positive Voltage-IG Fuse 20A
3 | RED/BLU | Tail Relay Control
4 | GRN/RED | Left Turn Signal
5 | GRN/YEL | Right Turn Signal
6 | YEL/BLU | Ignition Positive Voltage-WIP Fuse 15A